{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Dimensionet","Njësia","","Lartësia","mm","550","550","734"]
["","","","Gjerësia","mm","765","765","958"]
["","","","Thellësia","mm","285","285","340"]
["Pesha","Njësia","","","kg","36","41","60"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","500","500","420"]
["","","Ngrohje","Super e ulët","rpm","320","500","420"]
["Compressor","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","46","48"]
["","","","Nom.","dBA","","","48"]
["","Ngrohje","","I lartë","dBA","48","50"]
["","","","Nom.","dBA","","","48.0"]
["Agjenti ftohës","Lloji","","","","R-32","R-32","R-32"]
["","Mbushja","","","kg","0.88","1.15","2"]
["","Mbushja","","","tCO2Eq","0.60","0.78","1.35"]
["","GWP","","","","675","675","675.0"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","20","20","25"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 20m)","0.02 (për gjatësinë e tubave që kalojnë 20m)","0.02 (për gjatësinë e tubave që kalojnë 30 m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","15.0","15.0","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","30","30","50"]
["Aksesore Standarde","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50"]
["","Tensioni","","","V","220-230-240","220-230-240","220-240"]
["Shënime","","","","","(1) - Për një dhomë","(1) - Për një dhomë","(1) - Për një dhomë"]
["Aksesore Standarde","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]