{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Niveli i presionit të zhurmës","Ngrohje","","Nom.","dBA","48","48","","50","50"]
["","Ftohje","","Nom.","dBA","47","47","","48","48"]
["Aksesore Standarde","Manual instalimi","","","","1","1","","1","1"]
["","Qese vidash","","","","1","1","","1","1"]
["","Tapë kullimi","","","","1","1","","1","1"]
["","Komplet reduktorësh","","","","","","","1","1"]
["Agjenti ftohës","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Mbushja","","","kg","1.20","1.20","","1.60","1.60"]
["","Lloji","","","","R-410A","R-410A","","R-410A","R-410A"]
["Piping connections","Ndryshimi i nivelit","IU - IU","Maks.","m","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Maks.","m","15","15","","15","15"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 20m)","0.02 (për gjatësinë e tubave që kalojnë 20m)","","0.02 (për gjatësinë e tubave që kalojnë 20m)","0.02 (për gjatësinë e tubave që kalojnë 20m)"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","30","30","","30","30"]
["Kompresori","Type","","","","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht","","Kompresor me lëkundje i izoluar hermetikisht","Kompresor me lëkundje i izoluar hermetikisht"]
["Dimensionet","Njësia","","Gjerësia","mm","765","765","","765","765"]
["","","","Thellësia","mm","285","285","","285","285"]
["","","","Lartësia","mm","550","550","","550","550"]
["Pesha","Njësia","","","kg","38","38","","42","42"]
["Power supply","Phase","","","","1~","1~","","1~","1~"]
["","Frekuenca","","","Hz","50","50","","50","50"]
["","Tensioni","","","V","220-240","220-240","","220-240","220-240"]
["Shënime","","","","","(1) - Përmban gaze të fluorinuara të efektit serrë","(1) - Përmban gaze të fluorinuara të efektit serrë","","(1) - Përmban gaze të fluorinuara të efektit serrë","(1) - Përmban gaze të fluorinuara të efektit serrë"]
["Dimensionet","Njësia","","Lartësia","mm","","","550","","","550"]
["","","","Gjerësia","mm","","","765","","","765"]
["","","","Thellësia","mm","","","285","","","285"]
["Pesha","Njësia","","","kg","","","38","","","42"]
["Kompresori","Type","","","","","","Kompresor rrotullues i mbyllur hermetikisht","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","","","10","","","10"]
["","","","Maks.","°CDB","","","46","","","46"]
["","Ngrohje","Ambienti","Min.","°CWB","","","-15","","","-15"]
["","","","Maks.","°CWB","","","15.5","","","15.5"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","","","47","","","48"]
["","Ngrohje","","Nom.","dBA","","","48","","","50"]
["Agjenti ftohës","Lloji","","","","","","R-410A","","","R-410A"]
["","Mbushja","","","kg","","","1.20","","","1.60"]
["","Mbushja","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","","","20","","","20"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","","","0.02 (për gjatësinë e tubave që kalojnë 20m)","","","0.02 (për gjatësinë e tubave që kalojnë 20m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","","","15","","","15"]
["","","IU - IU","Maks.","m","","","7.5","","","7.5"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","","","30","","","30"]
["Aksesore Standarde","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Furnizimi me energji","Faza","","","","","","1~","","","1~"]
["","Frekuenca","","","Hz","","","50","","","50"]
["","Tensioni","","","V","","","220-240","","","220-240"]
["Aksesore Standarde","Reducer assembly","","","","","","","","","1"]