{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-A"]
[]
[]
[]
[]
["","","","","","3MXM40A2V1B","3MXM52A2V1B","3MXM68A2V1B"]
["Dimensionet","Njësia","","Lartësia","mm","734","734","734"]
["","","","Gjerësia","mm","974","974","974"]
["","","","Thellësia","mm","408","408","408"]
["Pesha","Njësia","","","kg","57","57","62"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","46","46","48"]
["","Ngrohje","","Nom.","dBA","47","47","48"]
["Agjenti ftohës","Lloji","","","","R-32","R-32","R-32"]
["","Mbushja","","","kg","1.8","1.8","2"]
["","Mbushja","","","tCO2Eq","1.22","1.22","1.35"]
["","GWP","","","","675","675","675"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","25 (1)","25","25 (1)"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 30 m)","0.02 (për gjatësinë e tubave që kalojnë 30 m)","0.02 (për gjatësinë e tubave që kalojnë 30 m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","15","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","50 (2)","50","50"]
["Aksesore Standarde","Installation manual","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["","Reducer assembly","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240"]
["Shënime","","","","","(1) - Për një dhomë","(1) - Për një dhomë"]
["","","","","","(2) - Për kombinim me CVXM-A, FVXM-A - gjatësia minimale e tubacioneve është 30 m.","(2) - Për kombinim me CVXM-A, FVXM-A - gjatësia minimale e tubacioneve është 30 m."]
["","","","","","","","(1) - Për një dhomë"]