{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-M"]
[]
[]
[]
[]
["","","","","","3MXM40M2V1B","3MXM52M2V1B","3MXM68M2V1B"]
["Ventilatori","Shkalla e qarkullimit të ajrit","Ftohje","Super e ulët","m³/min","24","24","24.1"]
["","","Ngrohje","Super e ulët","m³/min","24","24","24.1"]
["","","","Super e ulët","cfm","847","847","851"]
["","","Ngrohje","Super e ulët","cfm","847","847","851"]
["Dimensionet","Njësia","","Lartësia","mm","734","734","734"]
["","","","Gjerësia","mm","868","868","868"]
["","","","Thellësia","mm","320","320","320"]
["Pesha","Njësia","","","kg","57","57","62"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","420","420"]
["","","Ngrohje","Super e ulët","rpm","420","420"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Ngrohje","Ambienti","Min.","°CWB","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","46","46","48"]
["","Ngrohje","","Nom.","dBA","47","47","48"]
["Agjenti ftohës","Lloji","","","","R-32","R-32","R-32"]
["","Mbushja","","","kg","1.80","1.80","2.0"]
["","Mbushja","","","tCO2Eq","1.2","1.2","1.4"]
["","GWP","","","","675","675","675"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","25","25","25"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 30 m)","0.02 (për gjatësinë e tubave që kalojnë 30 m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","15","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","50","50"]
["Aksesore Standarde","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240"]
["Kompresori","Lloji","","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Aksesore Standarde","Drain cap","","","","","","9"]
["","Reducer assembly","","","","","","1"]