{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N8"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B8","3MXM52N2V1B8"]
["Dimensionet","Njësia","","Lartësia","mm","734","734"]
["","","","Gjerësia","mm","974","974"]
["","","","Thellësia","mm","401","401"]
["Pesha","Njësia","","","kg","57","57"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","420","420"]
["","","Ngrohje","Super e ulët","rpm","420","420"]
["Compressor","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","46","46"]
["","Ngrohje","","Nom.","dBA","47.0","47.0"]
["Agjenti ftohës","Lloji","","","","R-32","R-32"]
["","Mbushja","","","kg","1.8","1.8"]
["","Mbushja","","","tCO2Eq","1.22","1.22"]
["","GWP","","","","675.0","675.0"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","25","25"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 30 m)","0.02 (për gjatësinë e tubave që kalojnë 30 m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","15.0","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","50","50"]
["Aksesore Standarde","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]
["Shënime","","","","","(1) - Për një dhomë","(1) - Për një dhomë"]
["","","","","","(2) - Për kombinim me CVXM-A, FVXM-A - gjatësia minimale e tubacioneve është 30 m.","(2) - Për kombinim me CVXM-A, FVXM-A - gjatësia minimale e tubacioneve është 30 m."]