{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":8,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXS-E"]
[]
[]
[]
[]
["","","","","","5MXS90E3V3B2","5MXS90E3V3B","5MXS90E7V3B"]
["Niveli i presionit të zhurmës","Ngrohje","","Nom.","dBA","52","52"]
["","Ftohje","","Nom.","dBA","52","52"]
["Aksesore Standarde","Manual instalimi","","","","1","1"]
["","Tapë kullimi","","","","1","1"]
["","Komplet reduktorësh","","","","1","1"]
["Agjenti ftohës","Charge","","","TCO2Eq","6.2","6.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Mbushja","","","kg","2.99","2.99"]
["","Lloji","","","","R-410A","R-410A"]
["Gama e funksionimit","Ftohja","Ambienti","Maks.","°CDB","46"]
["","","","Min.","°CDB","-10"]
["","Ngrohje","Ambienti","Maks.","°CWB","18"]
["","","","Min.","°CWB","-15"]
["Piping connections","Ndryshimi i nivelit","IU - IU","Maks.","m","7.5"]
["","","IU - OU","Maks.","m","15"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 30 m)"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","75"]
["Kompresori","Type","","","","Kompresor me lëkundje i izoluar hermetikisht"]
["Dimensionet","Njësia","","Gjerësia","mm","900","900"]
["","","","Thellësia","mm","320","320"]
["","","","Lartësia","mm","770","770"]
["Pesha","Njësia","","","kg","73","73"]
["Power supply","Phase","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","230","230"]
["Shënime","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19.0°CWB; temperatura e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7.5m","(1) - Ftohje: temp. e brendshme 27°CDB, 19.0°CWB; temperatura e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7.5m"]
["","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7.5m","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7.5m"]
["","","","","","(3) - Përmban gaze të fluorinuara të efektit serrë","(3) - Përmban gaze të fluorinuara të efektit serrë"]
["Piping connections","Ndryshimi i nivelit","IU - IU","Maks.","m","","7.5"]
["","","IU - OU","Maks.","m","","15"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","","0.02 (për gjatësinë e tubave që kalojnë 30 m)"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","","75"]
["Kompresori","Type","","","","","Kompresor me lëkundje i izoluar hermetikisht"]
["Dimensionet","Njësia","","Lartësia","mm","","","770"]
["","","","Gjerësia","mm","","","900"]
["","","","Thellësia","mm","","","320"]
["Pesha","Njësia","","","kg","","","73"]
["Kompresori","Type","","","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["","Ngrohje","Ambienti","Min.","°CWB","","","-15"]
["","","","Maks.","°CWB","","","15.5"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","","","52"]
["","Ngrohje","","Nom.","dBA","","","52"]
["Agjenti ftohës","Lloji","","","","","","R-410A"]
["","Mbushja","","","kg","","","2.99"]
["","Mbushja","","","tCO2Eq","","","6.2"]
["","GWP","","","","","","2087.5"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","","","25"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","","","0.02 (për gjatësinë e tubave që kalojnë 30 m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","","","15"]
["","","IU - IU","Maks.","m","","","7.5"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","","","75"]
["Aksesore Standarde","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Furnizimi me energji","Faza","","","","","","1~"]
["","Frekuenca","","","Hz","","","50"]
["","Tensioni","","","V","","","230"]