{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5XXM-A"]
[]
[]
[]
[]
["","","","","","5XXM68A2V1B","5XXM90A2V1B"]
["Dimensionet","Njësia","","Lartësia","mm","734","734"]
["","","","Gjerësia","mm","1040","1040"]
["","","","Thellësia","mm","408","408"]
["Pesha","Njësia","","","kg","69.0","73.0"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","50","50"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","48.0 (2)","52.0 (2)"]
["","Ngrohje","","Nom.","dBA","49.0 (2), 51.0 (3)","53.0 (2), 55.0 (3)"]
["Agjenti ftohës","Lloji","","","","R-32","R-32"]
["","Mbushja","","","kg","2.00","2.40"]
["","Mbushja","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675.0"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","25 (5) (4)","25 (4) (5)"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 30 m)","0.02 (për gjatësinë e tubave që kalojnë 30 m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","15.0 (5)","15.0 (5)"]
["","","IU - IU","Maks.","m","7.5 (5)","7.5 (5)"]
["","Gjatësia totale e tubacioneve","Sistemi","Aktuale","m","60","75"]
["Aksesore Standarde","Installation manual","","","","1","1"]
["","Kapak kullimi","","","","3","3"]
["","Tapë kullimi","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["Gama e efikasitetit të energjisë","","","","","A+++ ~ D","A+++ ~ D"]
["Furnizimi me energji","Faza","","","","1~","1~"]
["","Frekuenca","","","Hz","50","50"]
["","Tensioni","","","V","220-240","220-240"]
["Shënime","","","","","(1) - Shiko skicat e veçanta për diapazonin e funksionimit","(1) - Shiko skicat e veçanta për diapazonin e funksionimit"]
["","","","","","(2) - For DX combination","(2) - For DX combination"]
["","","","","","(3) - For Space heating operation of CHVX07 unit","(3) - For Space heating operation of CHVX07 unit"]
["","","","","","(4) - Për një dhomë","(4) - Për një dhomë"]
["","","","","","(5) - For combination with FBA71/100/125 refer to installation manual","(5) - For combination with FBA71/100/125 refer to installation manual"]
["","","","","","(6) - Përmban gaze të fluorinuara të efektit serrë","(6) - Përmban gaze të fluorinuara të efektit serrë"]