{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Aksesore Standarde","Manual instalimi","","","","Manual instalimi"]
["","Manual përdorimi","","","","Manual përdorimi"]
["","Vida+Rondela","","","","Vida+Rondela"]
["","Telekomandë me valë","","","","Telekomandë me valë"]
["","Grila e kyçit të kapakut","","","","Grila e kyçit të kapakut"]
["","Bateria","","","","Bateria"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","9.52"]
["","Gazi","","Dia. jasht.","mm","15.88"]
["","Kullimi","","","","19.05"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.128"]
["","Ngrohje","","Nom.","kW","0.128"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","64"]
["","Ngrohje","","","dBA","64"]
["Dimensionet","Njësia","","Gjerësia","mm","600"]
["","","","Thellësia","mm","1,007"]
["","","","Lartësia","mm","285"]
["Veshja e jashtme","Materiali","","","","Çelik i galvanizuar"]
["Pesha","Njësia","","","kg","35"]
["Ventilatori","Presioni i jashtëm statik","","I lartë","Pa","90"]
["","","","Nom.","Pa","77"]
["","","","I ulët","Pa","64"]
["Power supply","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Emri","","","","V1"]
["","Tensioni","","","V","220-240"]
["Fuqia në hyrje","Ngrohje","","Nom.","kW","","0.109"]
["","Ftohje","","Nom.","kW","","0.109"]
["Ventilatori","Presioni i jashtëm statik","","I lartë","Pa","","70","150","150"]
["","","","I ulët","Pa","","45","111","92"]
["Veshja e jashtme","Materiali","","","","","Çelik i galvanizuar"]
["Dimensionet","Njësia","","Lartësia","mm","","378","378","378"]
["","","","Gjerësia","mm","","541","1300","1500"]
["","","","Thellësia","mm","","1045","541","541"]
["Pesha","Njësia","","","kg","","44","50","56"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37","44"]
["","","","I ulët","m³/min","","18.3","34.8","37.9"]
["","","Ngrohje","I lartë","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37.4","43.9"]
["","","","I ulët","m³/min","","18.3","34.8","37.9"]
["","Presioni i jashtëm statik","","Nom.","Pa","","57","128","122"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","60","72","73"]
["","Ngrohje","","","dBA","","60","72","73"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","I ulët","dBA","","36","50","50"]
["","Ngrohje","","I lartë","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","I ulët","dBA","","36","50","50"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","9.52","9.52","9.52"]
["","Gazi","","Dia. jasht.","mm","","15.88","15.9","15.9"]
["","Kullimi","","","","","19.05"]
["Aksesore Standarde","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Furnizimi me energji","Faza","","","","","1~"]
["","Frekuenca","","","Hz","","50"]
["","Tensioni","","","V","","220-240"]
["Kapaciteti ftohës","Kapaciteti total","","Nom.","kW","","","12.10","13.00"]
["Kapaciteti i ngrohjes","Kapaciteti total","","Nom.","kW","","","13.5","15.5"]
["Veshja e jashtme","Ngjyra","","","","","","Pllakë me çelik të galvanizuar / Jo i lyer","Pllakë me çelik të galvanizuar / Jo i lyer"]
["Ventilatori","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","","","37","44"]
["","","Ngrohje","Mesatar","m³/min","","","37.4","43.9"]
["Niveli i presionit të zhurmës","Ftohje","","Mesatar","dBA","","","52","53"]
["","Ngrohje","","Mesatar","dBA","","","52","53"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","","","ARCWLA","ARCWLA"]