{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Funksionim pa zhurmë","dBA","","36","","41"]
["","","","I ulët","dBA","","38","","43"]
["","Ftohje","","Funksionim pa zhurmë","dBA","","36","","41"]
["","","","I ulët","dBA","","38","","43"]
["","","","I lartë","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Aksesore Standarde","Manual instalimi","","","","","Manual instalimi","","Manual instalimi"]
["","Manual përdorimi","","","","","Manual përdorimi","","Manual përdorimi"]
["","Vida","","","","","Vida","","Vida"]
["","Rondele","","","","","Rondele","","Rondele"]
["","Telekomandë me valë","","","","","Telekomandë me valë","","Telekomandë me valë"]
["","Grila e kyçit të kapakut","","","","","Grila e kyçit të kapakut","","Grila e kyçit të kapakut"]
["","Bateria","","","","","Bateria","","Bateria"]
["Sistemet e kontrollit","Telekomandë me tela","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","9.52","","9.52"]
["","Gazi","","Dia. jasht.","mm","","15.88","","15.88"]
["","Kullimi","","","","","19.05","","19.05"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","0.094","","0.137"]
["","Ngrohje","","Nom.","kW","","0.094","","0.137"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","56","","60"]
["","Ngrohje","","","dBA","","56","","60"]
["Dimensionet","Njësia","","Gjerësia","mm","","820","","820"]
["","","","Thellësia","mm","","820","","820"]
["","","","Lartësia","mm","","300","","300"]
["Veshja e jashtme","Materiali","","","","","Çelik i galvanizuar","","Çelik i galvanizuar"]
["Pesha","Njësia","","","kg","","39","","39"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","I lartë","m³/min","","29.2","","34.0"]
["","","","I ulët","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Ftohje","I ulët","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","I lartë","m³/min","","29.2","","34.0"]
["","","","Funksionim pa zhurmë","m³/min","","17.6","","22.1"]
["","","Ftohje","Funksionim pa zhurmë","m³/min","","17.6","","22.1"]
["Paneli dekorativ","Pesha","","","kg","","4","","4"]
["","Dimensionet","","Lartësia","mm","","82","","82"]
["","","","Thellësia","mm","","990","","990"]
["","","","Gjerësia","mm","","990","","990"]
["","Ngjyra","","","","","E bardhë","","E bardhë"]
["Power supply","Faza","","","","","1~","","1~"]
["","Emri","","","","","V1","","V1"]
["","Frekuenca","","","Hz","","50","","50"]
["","Tensioni","","","V","","220-240","","220-240"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","Funksionim pa zhurmë","m³/min","15","","22.1"]
["Fuqia në hyrje","Ngrohje","","Nom.","kW","0.067","","0.137"]
["","Ftohje","","Nom.","kW","0.067","","0.137"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","Funksionim pa zhurmë","m³/min","15","","22.1"]
["Veshja e jashtme","Materiali","","","","Çelik i galvanizuar","","Çelik i galvanizuar"]
["Dimensionet","Njësia","","Lartësia","mm","265","","300"]
["","","","Gjerësia","mm","820","","820"]
["","","","Thellësia","mm","820","","820"]
["Pesha","Njësia","","","kg","31","","39"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","I ulët","m³/min","17.6","","26.3"]
["","","Ngrohje","I lartë","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","I ulët","m³/min","17.6","","26.3"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","54","","60"]
["","Ngrohje","","","dBA","54","","60"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","I ulët","dBA","35","","43"]
["","","","Funksionim pa zhurmë","dBA","32","","41"]
["","Ngrohje","","I lartë","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","I ulët","dBA","35","","43"]
["","","","Funksionim pa zhurmë","dBA","32","","41"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","9.52","","9.52"]
["","Gazi","","Dia. jasht.","mm","15.88","","15.88"]
["","Kullimi","","","","19.05","","19.05"]
["Paneli dekorativ","Dimensionet","","Lartësia","mm","82","","82"]
["","","","Gjerësia","mm","990","","990"]
["","","","Thellësia","mm","990","","990"]
["","Pesha","","","kg","4","","4"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","ARCWLA","","ARCWLA"]
["","Telekomandë me tela","","","","ARCWB","","ARCWB"]
["Aksesore Standarde","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Furnizimi me energji","Faza","","","","1~","","1~"]
["","Frekuenca","","","Hz","50","","50"]
["","Tensioni","","","V","220-240","","220-240"]