{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS35L3V1B","ARXS25L3V1B (Archived)"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","48"]
["","","","I ulët","dBA","45"]
["Aksesore Standarde","1","","","","550"]
["Agjenti ftohës","Charge","","","kg","2.5"]
["","Lloji","","","","1.2"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","Super e ulët","m³/min","30.1"]
["","","","Super e ulët","cfm","1,063"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","740"]
["","","Ngrohje","Super e ulët","rpm","-15"]
["Diapazoni i funksionimit","Ngrohje","Ambienti","Min.","°CWB","20"]
["","","","Maks.","°CWB","10"]
["Niveli i presionit të zhurmës","Ftohje","","I ulët","dBA","44"]
["","","","I lartë","dBA","48"]
["Kompresori","Type","","","","Kompresor me lëkundje i izoluar hermetikisht"]
["Dimensionet","Njësia","","Gjerësia","mm","285"]
["","","","Thellësia","mm","612"]
["","","","Lartësia","mm","765"]
["Pesha","Njësia","","","kg","34"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ngrohje","Super e ulët","cfm","904"]
["","","","Super e ulët","m³/min","25.6"]
["Power supply","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","220-240"]
["Shënime","","","","","(1) - Përmban gaze të fluorinuara të efektit serrë","(1) - 220V"]
["","","","","","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 230V","(3) - 240V"]
["","","","","","(4) - 240V"]
["Ventilatori","Shkalla e qarkullimit të ajrit","Ftohje","Super e ulët","m³/min","","30.1"]
["","","Ngrohje","Super e ulët","m³/min","","25.6"]
["","","","Super e ulët","cfm","","1063"]
["","","Ngrohje","Super e ulët","cfm","","904"]
["Dimensionet","Njësia","","Lartësia","mm","","550"]
["","","","Gjerësia","mm","","765"]
["","","","Thellësia","mm","","285"]
["Pesha","Njësia","","","kg","","34"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Super e ulët","rpm","","780"]
["","","Ngrohje","Super e ulët","rpm","","740"]
["Kompresori","Lloji","","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","","10"]
["","","","Maks.","°CDB","","46"]
["","Ngrohje","Ambienti","Min.","°CWB","","-15"]
["","","","Maks.","°CWB","","18"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","46"]
["","Ngrohje","","I lartë","dBA","","47"]
["","","","I ulët","dBA","","44"]
["Agjenti ftohës","Lloji","","","","","R-410A"]
["","Mbushja","","","kg","","1.0"]
["","Mbushja","","","tCO2Eq","","2.1"]
["","GWP","","","","","2087.5"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","","20"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","","15"]
["Aksesore Standarde","Installation manual","","","","","1"]
["","Refrigerant charge label","","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1"]
["","Drain plug","","","","","1"]
["Furnizimi me energji","Faza","","","","","1~"]
["","Frekuenca","","","Hz","","50"]
["","Tensioni","","","V","","220-240"]