{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF42C5V1B","ATXF35C5V1B (Archived)"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","39.0","40.0","44.0"]
["","","","Mesatar","dBA","34.0","34.0","34.0"]
["","","","Funksionim pa zhurmë","dBA","21.0","21.0","22.0"]
["","","","I ulët","dBA","28.0","28.0","28.0"]
["","Ftohje","","Medium","dBA","33.0","33.0","36.0"]
["","","","Funksionim pa zhurmë","dBA","20.0","20.0","22.0"]
["","","","I ulët","dBA","25.0","26.0","30.0"]
["","","","I lartë","dBA","39.0","40.0","45.0"]
["Aksesore Standarde","Manual instalimi","","","","1","1","1"]
["","Manual përdorimi","","","","1","1","1"]
["","Bateri","","","","1","1","1"]
["","Telekomandë me rreze infra të kuqe","","","","1","1","1"]
["","Bateri AAA me qeliza të thata","","","","2","2","2"]
["","Mbajtës telekomande","","","","1","1","1"]
["","Pllakë montimi","","","","1","1","1"]
["","Vida mbërthimi për njësinë e brendshme","","","","2","2","2"]
["Sistemet e kontrollit","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1"]
["Lidhjet e tubacioneve","Liquid","","Dia. jasht.","mm","6.35","6.35","6.35"]
["","Gazi","","OD","mm","9.50","9.50","9.50"]
["","Kullimi","","","","18","18","18"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.023","0.023","0.040"]
["","Ngrohje","","Nom.","kW","0.023","0.023","0.040"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","53.0","54.0","59.0"]
["","Ngrohje","","","dBA","55.0","55.0","59.0"]
["Dimensionet","Njësia","","Gjerësia","mm","770","770","770"]
["","","","Thellësia","mm","225","225","225"]
["","","","Lartësia","mm","286","286","286"]
["Veshja e jashtme","Colour","","","","E bardhë","E bardhë","E bardhë"]
["Pesha","Njësia","","","kg","8.00","8.00","9.00"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50"]
["","Tensioni","","","V","220-440","220-440","220-440"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","","","0.029"]
["","Ngrohje","","Nom.","kW","","","","0.029"]
["Veshja e jashtme","Ngjyra","","","","","","","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","","","","286"]
["","","","Gjerësia","mm","","","","770"]
["","","","Thellësia","mm","","","","225"]
["Pesha","Njësia","","","kg","","","","8.5"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","","","","11.8"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","","","","8"]
["","","","I ulët","m³/min","","","","6.4"]
["","","","Funksionim pa zhurmë","m³/min","","","","4.4"]
["","","Ngrohje","I lartë","m³/min","","","","11.9"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","","","","8.6"]
["","","Ngrohje","I ulët","m³/min","","","","6.5"]
["","","","Funksionim pa zhurmë","m³/min","","","","5.3"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","","","54"]
["","Ngrohje","","","dBA","","","","56"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","","","43"]
["","","","Mesatar","dBA","","","","34"]
["","","","I ulët","dBA","","","","27"]
["","","","Funksionim pa zhurmë","dBA","","","","20"]
["","Ngrohje","","I lartë","dBA","","","","40"]
["","","","Mesatar","dBA","","","","35"]
["","","","I ulët","dBA","","","","29"]
["","","","Funksionim pa zhurmë","dBA","","","","21"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","","","6.35"]
["","Gazi","","Dia. jasht.","mm","","","","9.5"]
["","Kullimi","","","","","","","18"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","","","","ARC470A1"]
["","Telekomandë me tela","","","","","","","BRC073A1"]
["Aksesore Standarde","Installation manual","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","Operation manual","","","","","","","1"]
["","Batteries","","","","","","","1"]
["","Indoor unit fixing screws","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Mounting plate","","","","","","","1"]
["","Remote control holder","","","","","","","1"]
["Furnizimi me energji","Faza","","","","","","","1~"]
["","Frekuenca","","","Hz","","","","50"]
["","Tensioni","","","V","","","","220-440"]