{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F / ARXF-A"]
[]
[]
[]
[]
["","","","","ATXF50F5V1B / ARXF50A5V1B"]
["Outdoor unit","","","","ARXF50A5V1B"]
["Kapaciteti ftohës","Min.","","kW","1.7"]
["","Nom.","","kW","5"]
["","Maks.","","kW","6"]
["Kapaciteti ngrohës","Min.","","kW","1.7"]
["","Nom.","","kW","6"]
["","Maks.","","kW","7.7"]
["Efikasiteti nominal","EER","","","3.3"]
["","COP","","","3.71"]
["","Konsumi vjetor i energjisë","","kWh","283"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","A"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","A++"]
["","Kapaciteti","Pdesign","kW","5"]
["","SEER","","","6.18"]
["","Konsumi vjetor i energjisë","","kWh/a","283"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","A+"]
["","Kapaciteti","Pdesign","kW","4.6"]
["","SCOP/A","","","4.03"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","4.06"]
["","Konsumi vjetor i energjisë","","kWh/a","1598"]
["Shënime","","","","(1) - Kapacitetet nominale të ftohjes bazohen te: temperatura e brendshme: 27°CDB, 19°CWB, temperatura e jashtme: 35°CDB, tubacioni ekuivalent i agjentit ftohës: 5 m, diferenca e nivelit: 0 m. Të dhënat për seritë me efikasitet të lartë, certifikuar nga Eurovent"]
["","","","","(2) - Kapacitetet nominale të ngrohjes bazohen te: temperatura e brendshme: 20°CDB, temperatura e jashtme: 7°CDB, 6°CWB, tubacioni ekuivalent i agjentit ftohës: 5 m, diferenca e nivelit: 0 m. Të dhënat për seritë me efikasitet standard"]
["","","","","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]