{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-F"]
[]
[]
[]
[]
["","","","","","ATXF50F5V1B"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.04"]
["","Ngrohje","","Nom.","kW","0.04"]
["Veshja e jashtme","Ngjyra","","","","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","286"]
["","","","Gjerësia","mm","770"]
["","","","Thellësia","mm","225"]
["Pesha","Njësia","","","kg","9"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","12.6"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","9"]
["","","","I ulët","m³/min","7.2"]
["","","","Funksionim pa zhurmë","m³/min","6.4"]
["","","Ngrohje","I lartë","m³/min","12.8"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","9.6"]
["","","Ngrohje","I ulët","m³/min","7.2"]
["","","","Funksionim pa zhurmë","m³/min","6.4"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","59"]
["","Ngrohje","","","dBA","59"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","45"]
["","","","Mesatar","dBA","39"]
["","","","I ulët","dBA","34"]
["","","","Funksionim pa zhurmë","dBA","31"]
["","Ngrohje","","I lartë","dBA","44"]
["","","","Mesatar","dBA","38"]
["","","","I ulët","dBA","33"]
["","","","Funksionim pa zhurmë","dBA","30"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6"]
["","Gazi","","Dia. jasht.","mm","12.7"]
["","Kullimi","","","","18"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","ARC480A93"]
["","Telekomandë me tela","","","","BRC073A1"]
["Aksesore Standarde","ATXF50F5V1B","","","","1"]
["","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Furnizimi me energji","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","220-440"]
["Shënime","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m"]
["","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m (horizontal)"]
["","","","","","(3) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]