{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-A / ARXM-A"]
[]
[]
[]
[]
["","","","","ATXM25A2V1B / ARXM25A5V1B","ATXM25A5V1B / ARXM25A5V1B","ATXM35A2V1B / ARXM35A5V1B","ATXM35A5V1B / ARXM35A5V1B","ATXM50A2V1B / ARXM50A5V1B","ATXM50A5V1B / ARXM50A5V1B"]
["Kapaciteti ftohës","Min.","","kW","0.90","0.90","0.90","0.90","1.70","1.70"]
["","Nom.","","kW","2.50","2.50","3.50","3.50","5.00","5.00"]
["","Maks.","","kW","3.80","3.80","4.40","4.40","5.30","5.30"]
["Kapaciteti ngrohës","Min.","","kW","0.80","0.80","0.80","0.80","1.70","1.70"]
["","Nom.","","kW","2.80","2.80","4.00","4.00","5.80","5.80"]
["","Maks.","","kW","5.00","5.00","5.50","5.50","6.50","6.50"]
["Efikasiteti nominal","EER","","","5.10","5.10","4.50","4.50","3.58","3.58"]
["","COP","","","5.00","5.00","4.45","4.45","4.05","4.05"]
["","Konsumi vjetor i energjisë","","kWh","245","245","389","389","698","698"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A","A","A","A","A","A"]
["","","Ngrohje","","A","A","A","A","A","A"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","A+++","A+++","A+++","A+++","A++","A++"]
["","Kapaciteti","Pdesign","kW","2.50","2.50","3.50","3.50","5.00","5.00"]
["","SEER","","","9.30","9.30","9.10","9.10","7.65","7.65"]
["","Konsumi vjetor i energjisë","","kWh/a","94","94","135","135","229","229"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","A+++","A+++","A+++","A+++","A++","A++"]
["","Kapaciteti","Pdesign","kW","2.40","2.40","2.50","2.50","4.50","4.50"]
["","SCOP/A","","","5.15","5.15","5.15","5.15","4.75","4.75"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","2.40","2.40","2.50","2.50","4.50","4.50"]
["","Konsumi vjetor i energjisë","","kWh/a","652","652","679","679","1326","1326"]