{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDW"]
[]
[]
[]
[]
["","","","","BRC1HHDAW (Archived)"]
["Veshja e jashtme","Ngjyra","","","E bardhë"]
["Mbulesa","Mbulesa e butonave","","","Jo"]
["","Funksionimi LED","Ngjyra","","Treguesi blu i statusit"]
["Dimensionet","Njësia","Lartësia","mm","85"]
["","","Gjerësia","mm","85"]
["","","Thellësia","mm","25"]
["","Njësia e ambalazhuar","Lartësia","mm","50"]
["","","Gjerësia","mm","217"]
["","","Thellësia","mm","161"]
["Pesha","Njësia","","kg","0.110"]
["","Njësia e ambalazhuar","","kg","0.317"]
["Ambalazhimi","Materiali","","","Karton"]
["","Pesha","","kg","0.0850"]
["LCD","Lloji","","","100 x 150 pika"]
["","Dimensionet","Lartësia","mm","40.7"]
["","","Gjerësia","mm","28.0"]
["","Drita e pasme","Ngjyra","","E bardhë"]
["Temperatura e ambientit","Funksionimi","Min.","°C","-10"]
["","","Maks.","°C","52"]
["","Ruajtja","Min.","°C","-20"]
["","","Maks.","°C","70"]
["","Temperatura e ambientit-=-Lagështia relative <-=-%","","%","95"]
["Sisteme kontrolli","Kategoria e kontrollit të temperaturës","","","VI"]
["","Kontributi në efikasitetin sezonal të ngrohjes së ambientit","","%","4.0"]
["Lidhjet e telave","Gjatësia e instalimeve","Maks.","m","500"]