{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Niveli i presionit të zhurmës","Ngrohje","I lartë","dBA","39"]
["","","Mesatar","dBA","32"]
["","","Funksionim pa zhurmë","dBA","21"]
["","","I ulët","dBA","25"]
["","Ftohje","Mesatar","dBA","32"]
["","","Funksionim pa zhurmë","dBA","21"]
["","","I ulët","dBA","25"]
["","","I lartë","dBA","39"]
["Aksesore Standarde","Manual instalimi","","","1"]
["","Manual përdorimi","","","1"]
["","Filtër ajri","","","2"]
["","Telekomandë me rreze infra të kuqe","","","1"]
["","Pllakë montimi telekomande","","","1"]
["","Qese vidash","","","1"]
["","Mbulesa e vidës","","","1"]
["","Bateri AAA me qeliza të thata","","","2"]
["","Masat e përgjithshme të sigurisë","","","1"]
["Agjenti ftohës","GWP","","","675.0"]
["Sisteme kontrolli","Wired remote control","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","6.35"]
["","Gazi","Dia. jasht.","mm","9.50"]
["","Kullimi","","","18"]
["Fuqia në hyrje","Ftohje","Nom.","kW","0.020"]
["","Ngrohje","Nom.","kW","0.020"]
["Sound power level","Ftohje","","dBA","57"]
["Dimensionet","Njësia","Gjerësia","mm","798"]
["","","Thellësia","mm","189"]
["","","Lartësia","mm","295"]
["Veshja e jashtme","Ngjyra","","","Dru i zi"]
["Pesha","Njësia","","kg","12"]
["Power supply","Faza","","","1~"]
["","Frekuenca","","Hz","50"]
["","Emri","","","V1"]
["","Tensioni","","V","220-240"]