{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BT"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BT"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","39"]
["","","","Mesatar","dBA","32"]
["","","","Funksionim pa zhurmë","dBA","21"]
["","","","I ulët","dBA","25"]
["","Ftohje","","Mesatar","dBA","32"]
["","","","Funksionim pa zhurmë","dBA","21"]
["","","","I ulët","dBA","25"]
["","","","I lartë","dBA","39"]
["Aksesore Standarde","Manual instalimi","","","","1"]
["","Manual përdorimi","","","","1"]
["","Filtër ajri","","","","2"]
["","Telekomandë me rreze infra të kuqe","","","","1"]
["","Pllakë montimi telekomande","","","","1"]
["","Qese vidash","","","","1"]
["","Mbulesa e vidës","","","","2"]
["","Bateri AAA me qeliza të thata","","","","2"]
["","Masat e përgjithshme të sigurisë","","","","1"]
["Antipiretik","GWP","","","","675.0"]
["Control systems","Wired remote control","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Piping connections","Liquid","","Dia. jasht.","mm","6.35"]
["","Gas","","Diametri i jashtëm","mm","9.50"]
["","Kullimi","","","","18"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.020"]
["","Ngrohje","","Nom.","kW","0.020"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","57"]
["Dimensionet","Njësia","","Gjerësia","mm","798"]
["","","","Thellësia","mm","189"]
["","","","Lartësia","mm","295"]
["Veshja e jashtme","Colour","","","","Dru i zi"]
["Pesha","Njësia","","","kg","11.5"]
["Ventilatori","Shkalla e qarkullimit të ajrit","Ngrohje","I lartë","m³/min","10.9"]
["","","","Mesatar","m³/min","8.7"]
["","","","I ulët","m³/min","6.4"]
["","","","Funksionim pa zhurmë","m³/min","4.5"]
["","","Ftohje","I ulët","m³/min","6.1"]
["","","","Mesatar","m³/min","8.2"]
["","","","I lartë","m³/min","11.0"]
["","","","Funksionim pa zhurmë","m³/min","4.6"]
["Power supply","Phase","","","","1~"]
["","Name","","","","V1"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","220-240"]