{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCS601C51"]
[]
[]
[]
[]
["","","","","","DCS601C51."]
["Hyrja","Lloji","","","","Panel me prekje (hyrje analoge e koduar 10 bit)"]
["Temperatura e ambientit","Lagështia relative <","","","%","85"]
["","Funksionimi","","Min.","°C","0"]
["","","","Maks.","°C","40"]
["Numri maksimal i njësive të brendshme që lidhen","","","","","64, 128 (1)"]
["Komunikimi","DIII-NET","","Sasia","","1"]
["","","","Shënime","","Linja e komunikimit të pajisjeve të ajrit të kondicionuar"]
["","10BASE-T","","Shënime","","Opsioni i uebit"]
["","Eternet","","Shënime","","Portë për aksesin në ueb dhe funksionin e emailit"]
["","Terminali i hyrjes","Dixhital","Sasia","","1"]
["","","","Shënime","","Fikje e detyruar"]
["","","Seri impulsesh","Sasia","","3"]
["","","","Shënime","","Pulsi i matjes së fuqisë"]
["","Modem","","Shënime","","Mundësia për modem në bord"]
["","PCMCIA","","Shënime","","Kartë memorieje flash"]
["","RS-232C","","Shënime","","Përshtatësi DIII-NET plus"]
["Dimensionet","Njësia","","Gjerësia","mm","230"]
["","","","Thellësia","mm","107"]
["","","","Lartësia","mm","147"]
["LCD","Lloji","","","","QVGA (320 x 240), 4,096 ngjyra"]
["","Dimensionet","","Gjerësia","inç","5.7"]
["Numri maksimal i njësive të jashtme që lidhen","","","","","10, 20 (1)"]
["Power supply","Frekuenca","","","Hz","50/60"]
["","Tensioni","","","V","100-240 (furnizuar nga jashtë)"]
["Shënime","","","","","(1) - Kombinuar me DCS601A51"]