{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Niveli i presionit të zhurmës","Nom.","","","dBA","32.0 (6)"]
["Antipiretik","GWP","","","","2,090"]
["","Ngarkesa","","","kg","1.80"]
["","Type","","","","R-410A"]
["Diapazoni i funksionimit","Hapësira e instalimit","","Min.","°C","5.00"]
["","","","Maks.","°C","30.0"]
["","Ngrohje","Ana e ujit","Maks.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Ana e solucionit me kripë","","Min.","°C","-5.00"]
["","","","Maks.","°C","20.0"]
["","Ujë i ngrohtë në shtëpi","Ana e ujit","Maks.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Fuqia në hyrje","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Niveli i fuqisë së zhurmës","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Dimensionet","Njësia","","Gjerësia","mm","600"]
["","","","Thellësia","mm","728"]
["","","","Lartësia","mm","1,730"]
["Casing","Material","","","","Fletë metalike e ngjyrosur më parë"]
["","Ngjyra","","","","E bardhë"]
["Tank","Vëllimi i ujit","","","l","180"]
["","Mbrojtje nga gërryerja","","","","Anodë"]
["","Izolimi","","Humbja e nxehtësisë","kWh/24h","1.36 (4)"]
["Pesha","Njësia","","","kg","210"]
["Ngrohja e ambientit","Dalja e ujit klimë mesatare 35°C","Të përgjithshme","ηs (Efikasiteti sezonal i ngrohjes së ambientit)","%","194"]
["","","","Klas. efikasitetit të ngrohjes sezonale të ambientit","","A+++"]
["","","","SCOP","","5.06"]
["","Dalja e ujit klimë mesatare 55°C","Të përgjithshme","Seasonal space heating eff. class","","A++"]
["","","","ηs (Efikasiteti sezonal i ngrohjes së ambientit)","%","139"]
["","","","SCOP","","3.68"]
["Kapaciteti ngrohës","Nom.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Maks.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Faza","","","","3~"]
["","Name","","","","9W"]
["","Frekuenca","","","Hz","50"]
["","Voltage","","","V","400"]
["Rryma","Siguresat e rekomanduara","","","A","25"]
["Shënime","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45℃ (DT=5°C)"]
["","","","","","(3) - me 40% propilen glikoli"]
["","","","","","(4) - Humbja e nxehtësisë sipas EN12897"]
["","","","","","(5) - Duke përfshirë tubat + PHE + ngrohësin rezervë; me përjashtim të enës së zgjerimit"]
["","","","","","(6) - Niveli i presionit të zhurmës matet përmes një mikrofoni në një distancë prej 1m nga njësia. Është një vlerë relative, në varësi të distancës dhe ambientit akustik."]
["","","","","","(7) - Me pompë ngrohëse"]
["","","","","","(8) - Me pompë ngrohëse + ngrohës rezervë"]
["","","","","","(9) - Me ngrohës rezervë"]