{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERSQ-AY1"]
[]
[]
[]
[]
["","","","","","ERSQ011AAY1","ERSQ014AAY1","ERSQ016AAY1"]
["Niveli i presionit të zhurmës","Ngrohje","","Nom.","dBA","52","53","55"]
["Aksesore Standarde","Manual instalimi","","","","1","1","1"]
["Agjenti ftohës","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Ngarkesa","","","kg","4.5","4.5","4.5"]
["","Lloji","","","","R-410A","R-410A","R-410A"]
["Diapazoni i funksionimit","Ngrohje","","Maks.","°CWB","20","20","20"]
["","","","Min.","°CWB","-20","-20","-20"]
["","Ujë i ngrohtë në shtëpi","","Min.","°CDB","-20","-20","-20"]
["","","","Maks.","°CDB","35","35","35"]
["Lidhjet e tubacioneve","Termoizolimi","","","","Tuba lëngu dhe gazi","Tuba lëngu dhe gazi","Tuba lëngu dhe gazi"]
["","Lëngu","","Dia. jasht.","mm","9.52","9.52","9.52"]
["","Gazi","","Dia. jasht.","mm","15.9","15.9","15.9"]
["","Kullimi","","Diametri i jashtëm","mm","26x3","26x3","26x3"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","30","30","30"]
["Sound power level","Heating","","Nom.","dBA","68","69","71"]
["Dimensionet","Njësia","","Gjerësia","mm","900","900","900"]
["","","","Thellësia","mm","320","320","320"]
["","","","Lartësia","mm","1,345","1,345","1,345"]
["Pesha","Njësia","","","kg","120","120","120"]
["Power supply","Faza","","","","3~","3~","3~"]
["","Emri","","","","Y1","Y1","Y1"]
["","Frekuenca","","","Hz","50","50","50"]
["","Tensioni","","","V","380-415","380-415","380-415"]
["Rryma","Siguresat e rekomanduara","","","A","16","16","16"]
["Shënime","","","","","(1) - Shiko skicën e veçantë për diapazonin e funksionimit","(1) - Shiko skicën e veçantë për diapazonin e funksionimit","(1) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","","(2) - Ssc: Energjia e qarkut të shkurtër","(2) - Ssc: Energjia e qarkut të shkurtër","(2) - Ssc: Energjia e qarkut të shkurtër"]
["","","","","","(3) - Përmban gaze të fluorinuara të efektit serrë","(3) - Përmban gaze të fluorinuara të efektit serrë","(3) - Përmban gaze të fluorinuara të efektit serrë"]