{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWAA-DW1P-H"]
[]
[]
[]
[]
["","","","","","EWAA011DAW1P-H-","EWAA014DAW1P-H-","EWAA016DAW1P-H-"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","47.7","50.8","51.0"]
["Komponentët hidraulikë","Ena e zgjerimit","","Vëllimi","l","8","8","8"]
["Gama e funksionimit","Ana e ajrit","Ftohje","Min.","°CDB","10","10","10"]
["","","","Maks.","°CDB","43","43","43"]
["","Ana e ujit","Ftohje","Maks.","°CDB","22","22","22"]
["","","","Min.","°CDB","5","5","5"]
["Mbushja e agjentit ftohës","Për qark","","","kg","3.80","3.80","3.80"]
["","Refrigerant charge-=-Per circuit-=-TCO2Eq","","","TCO2Eq","2.6","2.6","2.6"]
["Kompresori","Type","","","","Kompresor rrotullues inverter i mbyllur hermetikisht","Kompresor rrotullues inverter i mbyllur hermetikisht","Kompresor rrotullues inverter i mbyllur hermetikisht"]
["","Starting method","","","","Drejtuar me inverter","Drejtuar me inverter","Drejtuar me inverter"]
["","Sasia","","","","1","1","1"]
["Shkëmbyesi i nxehtësisë së ajrit","Lloji","","","","Fletë me efikasitet të lartë dhe lloji i tubit me nën-ngrohës të integruar","Fletë me efikasitet të lartë dhe lloji i tubit me nën-ngrohës të integruar","Fletë me efikasitet të lartë dhe lloji i tubit me nën-ngrohës të integruar"]
["Pesha","Njësia","","","kg","147","147","147"]
["EER","","","","","3.26 (1), 5.31 (2)","3.16 (1), 5.04 (2)","3.06 (1), 4.74 (2)"]
["Antipiretik","GWP","","","","675.0","675.0","675.0"]
["","Lloji","","","","R-32","R-32","R-32"]
["","Qarqet","","Sasia","","1","1","1"]
["","Kontrolli","","","","Valvula elektronike e zgjerimit","Valvula elektronike e zgjerimit","Valvula elektronike e zgjerimit"]
["Motori i ventilatorit","Shpejtësia","Ftohje","Nom.","rpm","550","650","650"]
["Kapaciteti ftohës","Nom.","","","kW","11.6 (1), 11.5 (2)","12.8 (1), 12.7 (2)","14.0 (1), 15.3 (2)"]
["Shkëmbyesi i nxehtësisë së ujit","Vëllimi i ujit","","","l","2","2","2"]
["","Vëllimi minimal i ujit në sistem","","","l","20 (6)","20 (6)","20 (6)"]
["","Lloji","","","","Shkëmbyesi i nxehtësisë së pllakës","Shkëmbyesi i nxehtësisë së pllakës","Shkëmbyesi i nxehtësisë së pllakës"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","3.56 (1), 2.17 (2)","4.06 (1), 2.51 (2)","4.58 (1), 3.24 (2)"]
["Niveli i fuqisë së zhurmës","Ftohje","","Nom.","dBA","67.0","69.0","69.0"]
["Dimensionet","Njësia","","Gjerësia","mm","1,380","1,380","1,380"]
["","","","Thellësia","mm","460","460","460"]
["","","","Lartësia","mm","870","870","870"]
["Kontrolli i kapacitetit","Metoda","","","","E ndryshueshme (inverter)","E ndryshueshme (inverter)","E ndryshueshme (inverter)"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","Nom.","m³/min","70","85","85"]
["Kompresori","Starting method","","","","Inverteri","Inverteri","Inverteri"]
["Power supply","Faza","","","","3~","3~","3~"]
["","Frekuenca","","","Hz","50","50","50"]
["","Emri","","","","W1","W1","W1"]
["","Tensioni","","","V","400","400","400"]
["Shënime","","","","","(1) - Ftohje: EW 12°C; LW 7°C; kushtet e ambientit: 35°CDB","(1) - Ftohje: EW 12°C; LW 7°C; kushtet e ambientit: 35°CDB","(1) - Ftohje: EW 12°C; LW 7°C; kushtet e ambientit: 35°CDB"]
["","","","","","(2) - Ftohje: EW 23℃; LW 18℃; kushtet e ambientit: 35°CDB","(2) - Ftohje: EW 23℃; LW 18℃; kushtet e ambientit: 35°CDB","(2) - Ftohje: EW 23℃; LW 18℃; kushtet e ambientit: 35°CDB"]
["","","","","","(3) - Kushti: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Kushti: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Kushti: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Kushti: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - Kushti: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)","(4) - Kushti: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(5) - Sipas EN14825","(5) - Sipas EN14825","(5) - Sipas EN14825"]
["","","","","","(6) - Në varësi të regjimit të përdorimit, referojuni manualit të instalimit.","(6) - Në varësi të regjimit të përdorimit, referojuni manualit të instalimit.","(6) - Në varësi të regjimit të përdorimit, referojuni manualit të instalimit."]
["","","","","","(7) - Për më shumë detaje, shihni skicën e diapazonit të funksionimit","(7) - Për më shumë detaje, shihni skicën e diapazonit të funksionimit","(7) - Për më shumë detaje, shihni skicën e diapazonit të funksionimit"]