{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":13,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWFS-TZPSD"]
[]
[]
[]
[]
["","","","","","","EWFSH10TZPSD2","EWFSC10TZPSD2","EWFSH11TZPSD2","EWFSC12TZPSD2","EWFSH13TZPSD2","EWFSH14TZPSD2","EWFSH15TZPSD2"]
["Kapaciteti ftohës","Nom.","","","","kW","1381.36","1302.53","1446.85","1537.35","1785.62","1875.03","1970.53"]
["Kontrolli i kapacitetit","Metoda","","","","","Pa faza","Pa faza","Pa faza","Pa faza","Pa faza","Pa faza","Pa faza"]
["Kontrolli i kapacitetit","Kapaciteti minimal","","","","%","10.5","11.5","10.5","10","10","15","13.5"]
["Fuqia në hyrje","Ftohje","","","Nom.","kW","382.23","343.58","398.36","435.51","519.68","514.84","571.83"]
["EER","","","","","","3.61","3.79","3.63","3.53","3.44","3.64","3.45"]
["IPLV","","","","","","6.156","6.287","6.119","6.152","6.124","5.955","5.832"]
["SEER","","","","","","5.687","6.078","6.041","6.011","5.886","5.12","5.622"]
["Dimensionet","Njësia","","","Thellësia","mm","11200","11200","12280","12280","13360","13360","13360"]
["","","","","Lartësia","mm","2553","2553","2553","2553","2553","2553","2553"]
["","","","","Gjerësia","mm","2238","2238","2238","2238","2238","2238","2238"]
["Pesha","Pesha e funksionimit","","","","kg","9199","9189","9971","9976","11401","12085","12100"]
["Pesha","Njësia","","","","kg","7900","7900","8521","8521","9402","10070","10070"]
["Veshja e jashtme","Ngjyra","","","","","E bardhë fildishi","E bardhë fildishi","E bardhë fildishi","E bardhë fildishi","E bardhë fildishi","E bardhë fildishi","E bardhë fildishi"]
["Veshja e jashtme","Materiali","","","","","Fletë çeliku të galvanizuara dhe të lyera","Fletë çeliku të galvanizuara dhe të lyera","Fletë çeliku të galvanizuara dhe të lyera","Fletë çeliku të galvanizuara dhe të lyera","Fletë çeliku të galvanizuara dhe të lyera","Fletë çeliku të galvanizuara dhe të lyera","Fletë çeliku të galvanizuara dhe të lyera"]
["Shkëmbyesi i nxehtësisë së ujit - avulluesi","Lloji","","","","","Kuti dhe tubacion","Kuti dhe tubacion","Kuti dhe tubacion","Kuti dhe tubacion","Kuti dhe tubacion","Kuti dhe tubacion","Kuti dhe tubacion"]
["","Vëllimi i ujit","","","","l","481","481","557","557","1011","1011","1011"]
["Avullues-shkëmbyes i nxehtësisë me ujë","Rënia e presionit të ujit","","Ftohje","Nom.","kPa","50.7","46.31","54.24","54.07","40.62","43.54","47.34"]
["Shkëmbyesi i nxehtësisë së ajrit","Lloji","","","","","Mikro-kanal","Mikro-kanal","Mikro-kanal","Mikro-kanal","Mikro-kanal","Mikro-kanal","Mikro-kanal"]
["Ventilatori","Sasia","","","","","20","20","22","22","24","24","24"]
["","Lloji","","","","","Helikë direkte","Helikë direkte","Helikë direkte","Helikë direkte","Helikë direkte","Helikë direkte","Helikë direkte"]
["","Niveli i qarkullimit të ajrit","","Ftohje","Nom.","l/s","112550","112550","123805","123805","135060","135060","135060"]
["Motori i ventilatorit","Transmetimi","","","","","Pa karbonçina","Pa karbonçina","Pa karbonçina","Pa karbonçina","Pa karbonçina","Pa karbonçina","Pa karbonçina"]
["Kompresori","Sasia","","","","","2","2","2","2","2","2","2"]
["Kompresori","Lloji","","","","","Kompresor me vidë","Kompresor me vidë","Kompresor me vidë","Kompresor me vidë","Kompresor me vidë","Kompresor me vidë","Kompresor me vidë"]
["Diapazoni i funksionimit","Ana e ajrit","","Ftohje","Min.","°CDB","4","4","4","4","4","4","4"]
["","","","","Maks.","°CDB","18","18","18","18","18","18","18"]
["","Ana e ujit","","Diapazoni i funksionimit-=-Ana e ujit-=-Ftohje","Diapazoni i funksionimit-=-Ana e ujit-=-Ftohje-=-Min.-=-°CDB","°CDB","5","5","5","5","5","5","5"]
["","","","","Diapazoni i funksionimit-=-Ana e ujit-=-Ftohje-=-Maks.-=-°CDB","°CDB","42","42","42","42","42","42","42"]
["Niveli i fuqisë së zhurmës","Ftohje","","","Nom.","dBA","102.4","101.1","103","105.2","106.2","102","102.8"]
["Niveli i presionit të zhurmës","Ftohje","","","Nom.","dBA","77.3","76.6","77.4","77.7","78.9","78.9","79.7"]
["Agjenti ftohës","Lloji","","","","","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A"]
["Agjenti ftohës","GWP","","","","","630","630","630","630","630","630","630"]
["Agjenti ftohës","Agjenti ftohës-=-Ngarkesa-=-kg","","","","kg","150","140","160","165","190","205","220"]
["","Qarqet","","","Sasia","","2","2","2","2","2","2","2"]
["Lidhjet e tubacioneve","Hyrja/dalja e ujit të avulluesit (Diametri i jashtëm)","","","","","219.1","219.1","219.1","219.1","273","273","273"]
["Furnizimi me energji","Faza","","","","","3","3","3","3","3","3","3"]
["","Furnizimi me energji-=-Frekuenca","","","Frekuenca","","50","50","50","50","50","50","50"]
["","Furnizimi me energji-=-Tensioni","","","Tensioni","","400","400","400","400","400","400","400"]
["","Diapazoni i tensionit","","Min.","Min.","","-10","-10","-10","-10","-10","-10","-10"]
["","","","Maks.","Maks.","","10","10","10","10","10","10","10"]
["Njësia","Rryma e nisjes","","Njësia-=-Rryma e nisjes-=-Maks","Maks","","0","0","0","0","0","0","0"]
["","Rryma e punës","Ftohja","Njësia-=-Rryma e punës-=-Ftohja-=-Nom.","Nom.","","610","553","634","689","814","816","900"]
["","","","Njësia-=-Rryma e punës-=-Maks","Maks","","761","709","796","845","951","1039","1135"]
["","Njësia-=-Rryma maksimale e njësisë për madhësinë e telit","","","Rryma maksimale e njësisë për madhësinë e telit","","837","780","876","929","1021","1143","1248"]