{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FAA100BUV1B / RZASG100M7V1B","FAA71BUV1B / RZASG71M2V1B","FAA71BUV1B / FAA71BUV1B / RZASG140M7V1B"]
["Kapaciteti ftohës","Nom.","","kW","","6.80 (1)"]
["Ftohja e hapësirës","SEER","","","","6.41"]
["","Konsumi vjetor i energjisë","","kWh/a","","371"]
["","Kapaciteti","Pdesign","kW","","6.80"]
["","Kategoria e efikasitetit të energjisë","","","","A++"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","","4.50"]
["","SCOP/A","","","","3.90"]
["","Kategoria e efikasitetit të energjisë","","","","A"]
["","Konsumi vjetor i energjisë","","kWh/a","","1,615"]
["Kapaciteti ngrohës","Nom.","","kW","","7.50 (2)"]
["Kapaciteti ftohës","Nom.","","kW","9.5","","13.4"]
["Kapaciteti ngrohës","Nom.","","kW","10.8","","15.5"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","A+"]
["","Kapaciteti","Pdesign","kW","9.5","","13.4"]
["","SEER","","","5.83","","8.15"]
["","Konsumi vjetor i energjisë","","kWh/a","570","","986"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","A"]
["","Kapaciteti","Pdesign","kW","6","","7.80"]
["","SCOP/A","","","3.85","","4.53"]
["","Konsumi vjetor i energjisë","","kWh/a","2182","","2409"]
["Shënime","","","","","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temp. e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m.","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temp. e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m.","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","","(3) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","","(4) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]