{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAA100BUV1B / RZQSG100L8Y1B"]
["Kapaciteti ftohës","Nom.","","kW","9.5"]
["Ftohja e hapësirës","SEER","","","5.61"]
["","Konsumi vjetor i energjisë","","kWh/a","593"]
["","Kapaciteti","Pdesign","kW","9.50"]
["","Kategoria e efikasitetit të energjisë","","","A+"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","6.81"]
["","SCOP/A","","","4.01"]
["","Kategoria e efikasitetit të energjisë","","","A+"]
["","Konsumi vjetor i energjisë","","kWh/a","2,378"]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","1,578"]
["","EER","","","3.01"]
["","COP","","","3.41"]
["","Direktiva e etiketimit të energjisë","Ftohje","","B"]
["","","Ngrohje","","B"]
["Kapaciteti ngrohës","Nom.","","kW","10.8"]
["Shënime","","","","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temperatura e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","(3) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","(4) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]