{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RR-BV3"]
[]
[]
[]
[]
["","","","","FBA71A2VEB9 / RR71B8V3B","FBA71A2VEB9 / RR71B2V3B","FBA100A2VEB / RR100B8V3B"]
["Kapaciteti ftohës","Nom.","","kW","7.1 (1)","7.1 (1)","10.0 (1)"]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","1,351","1,351","1,915"]
["","EER","","","2.63","2.63","2.61"]
["","Direktiva e etiketimit të energjisë","Ftohje","","D","D","D"]
["Shënime","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m"]
["","","","","(2) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(2) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(2) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m"]
["","","","","(3) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7.5m (horizontalisht); diferenca e nivelit: 0m","(3) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7.5m (horizontalisht); diferenca e nivelit: 0m","(3) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7.5m (horizontalisht); diferenca e nivelit: 0m"]