{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RXS-L3"]
[]
[]
[]
[]
["","","","","FBQ35C8VEB / RXS35L3V1B"]
["Kapaciteti ftohës","Min.","","kW","1.4"]
["","Maks.","","kW","3.9"]
["","Nom.","","kW","3.40 (2)"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","6.35"]
["","Gazi","Diametri i jashtëm","mm","9.5"]
["","Kullimi","OD","mm","VP25 (Dia. i jashtëm 32, dia. i brendshëm 25)"]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","459"]
["","EER","","","3.70"]
["","COP","","","3.60"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","B"]
["Kapaciteti ngrohës","Nom.","","kW","4.00 (2)"]
["","Min.","","kW","1.3"]
["","Maks.","","kW","5.0"]
["Shënime","","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["","","","","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°"]
["","","","","(3) - 220V"]
["","","","","(4) - 230V"]
["","","","","(5) - 240V"]