{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RXS50L2V1B","FCAG60BVEB / RXS60L2V1B"]
["Kapaciteti ftohës","Nom.","","kW","5.00","5.70"]
["Kapaciteti ngrohës","Nom.","","kW","6.00","7.00"]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","EER","","","3.55","3.48"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A","A"]
["","","Ngrohje","","A","B"]
["Lidhjet e tubacioneve","Kullimi","Diametri i jashtëm","mm","VP25 (Dia. i jashtëm 32, dia. i brendshëm 25)","VP25 (Dia. i jashtëm 32, dia. i brendshëm 25)"]
["","Gazi","Dia. jasht.","mm","12.70","12.70"]
["","Lëngu","Dia. jasht.","mm","6.35","6.35"]
["Shënime","","","","(1) - Gjatë përdorimit normal: +22°C / + 32°C","(1) - Gjatë përdorimit normal: +22°C / + 32°C"]
["","","","","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m.","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","(3) - Shiko skicën e veçantë për diapazonin e funksionimit","(3) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","(4) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(4) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]