{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100HVEB / RZQG100L8Y1B","FCAHG125HVEB / RZQG125L8Y1B","FCAHG140HVEB / RZQG100L8Y1B","FCAHG140HVEB / RZQG125L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG100L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG125L8Y1B","FCAHG100HVEB / RZQG71L8Y1B","FCAHG71HVEB / RZQG71L8Y1B","FCAHG140HVEB / RZQG140L7Y1B"]
["Gama e efikasitetit të energjisë","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Kapaciteti ftohës","Nom.","","kW","","","","","","","6.80","6.80","13.40"]
["Ftohja e hapësirës","SEER","","","","","","","","","6.91","6.91","6.75"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","","345","345","1,191"]
["","Kapaciteti","Pdesign","kW","","","","","","","6.80","6.80","13.40"]
["","Kategoria e efikasitetit të energjisë","","","","","","","","","A++","A++"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","","","","","","","7.60","7.60","11.78"]
["","SCOP/A","","","","","","","","","4.54","4.54","4.38"]
["","Kategoria e efikasitetit të energjisë","","","","","","","","","A+","A+"]
["","Konsumi vjetor i energjisë","","kWh/a","","","","","","","2,344","2,344","3,766"]
["Efikasiteti nominal","EER","","","","","","","","","4.09","4.09","3.18"]
["Shënime","","","","","","","","","","(1) - Shiko skicën e veçantë për diapazonin e funksionimit","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temperatura e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m.","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temperatura e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","","","","","","","(2) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m.","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","","","","","","","","831"]
["","COP","","","","","","","","","","4.80","4.12"]
["","Direktiva e etiketimit të energjisë","Ftohje","","","","","","","","","A"]
["","","Ngrohje","","","","","","","","","A"]
["Kapaciteti ngrohës","Nom.","","kW","","","","","","","","7.50","15.50"]
["Shënime","","","","","","","","","","","(3) - Shiko skicën e veçantë për diapazonin e funksionimit","(3) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","","","","","","","","(4) - Shiko skicën e veçantë për të dhënat e skicave elektrike","(4) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["Ftohja e hapësirës","ηs,c","","%","","","","","","","","","266.88"]
["Ngrohja e hapësirës (klimë mesatare)","ηs,h","","%","","","","","","","","","172.10"]