{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":9,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H"]
[]
[]
[]
[]
["","","","","","FCAHG71HVEB","FCAHG100HVEB","FCAHG125HVEB","FCAHG140HVEB"]
["Kapaciteti ftohës","Kapaciteti total","","Nom.","kW","6.80","9.50","12.10","13.40"]
["Kapaciteti i ngrohjes","Kapaciteti total","","Nom.","kW","7.50","10.8","13.5","15.5"]
["Veshja e jashtme","Materiali","","","","Pllakë çeliku e galvanizuar","Pllakë çeliku e galvanizuar","Pllakë çeliku e galvanizuar","Pllakë çeliku e galvanizuar"]
["Dimensionet","Njësia","","Lartësia","mm","288","288","288","288"]
["","","","Gjerësia","mm","840","840","840","840"]
["","","","Thellësia","mm","840","840","840","840"]
["Pesha","Njësia","","","kg","25","25","25","25"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","23.6","32.2","34.4","34.4"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","18.8","25.7","27.3","27.3"]
["","","","I ulët","m³/min","13.7","19.1","21.2","21.2"]
["","","Ngrohje","I lartë","m³/min","23.6","30.8","32.1","32.1"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","18.8","24.6","25.5","25.5"]
["","","Ngrohje","I ulët","m³/min","13.7","18.3","19.7","19.7"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","53","61","61","61"]
["","Ngrohje","","","dBA","53","61","61","61"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","36","44","45","45"]
["","","","Mesatar","dBA","33","39","40","41"]
["","","","I ulët","dBA","29","33","35","37"]
["","Ngrohje","","I lartë","dBA","36","44","45","45"]
["","","","Mesatar","dBA","33","39","40","41"]
["","","","I ulët","dBA","29","33","35","37"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","9.52","9.52","9.52","9.52"]
["","Gazi","","Dia. jasht.","mm","15.9","15.9","15.9","15.9"]
["","Kullimi","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Paneli dekorativ","Modeli","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Dimensionet","","Lartësia","mm","65","65","65","65"]
["","","","Gjerësia","mm","950","950","950","950"]
["","","","Thellësia","mm","950","950","950","950"]
["","Pesha","","","kg","5.5","5.5","5.5","5.5"]
["Paneli dekorues 2","Modeli","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","Dimensionet","","Lartësia","mm","148","148","148","148"]
["","","","Gjerësia","mm","950","950","950","950"]
["","","","Thellësia","mm","950","950","950","950"]
["","Pesha","","","kg","10.3","10.3","10.3","10.3"]
["Paneli dekorues 3","Modeli","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Dimensionet","","Lartësia","mm","106","106","106","106"]
["","","","Gjerësia","mm","950","950","950","950"]
["","","","Thellësia","mm","950","950","950","950"]
["","Pesha","","","kg","6.5","6.5","6.5","6.5"]
["Sistemet e kontrollit","Infrared remote control","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]
["Sistemet e kontrollit","Telekomandë me tela","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Aksesore Standarde","Installation manual","","","","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8"]
["","Operation manual","","","","1","1","1","1"]
["","Wire clamp material","","","","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1"]
["","Clamps","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation guide","","","","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2"]
["","Screws","","","","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~","1~","1~"]
["","Furnizimi me energji-=-Frekuenca","","Frekuenca","","50/60","50/60","50/60","50/60"]
["","Furnizimi me energji-=-Tensioni","","Tensioni","","220-240/220","220-240/220","220-240/220","220-240/220"]