{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQHG100FVEB / RZQSG100L8Y1B","FCQHG125FVEB / RZQSG125L8Y1B","FCQHG140FVEB / RZQSG140L7Y1B"]
["Kapaciteti ftohës","Nom.","","kW","9.5","12.0","13.4"]
["Ftohja e hapësirës","SEER","","","6.7","5.4"]
["","Konsumi vjetor i energjisë","","kWh/a","497","778"]
["","Kapaciteti","Pdesign","kW","9.5","12"]
["","Kategoria e efikasitetit të energjisë","","","A++","A"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","8.03","8.03"]
["","SCOP/A","","","4.3","4.1"]
["","Kategoria e efikasitetit të energjisë","","","A+","A+"]
["","Konsumi vjetor i energjisë","","kWh/a","2,615","2,742"]
["Efikasiteti nominal","Annual energy consumption","","kWh","1,285","1,855"]
["","EER","","","3.70","3.23","3.21"]
["","COP","","","4.30","3.75","3.61"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A","A"]
["","","Ngrohje","","A","A"]
["Kapaciteti ngrohës","Nom.","","kW","10.8","13.5","15.5"]
["Shënime","","","","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së","(1) - EER/COP sipas Eurovent 2012, vetëm për përdorim jashtë BE-së"]
["","","","","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°","(2) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°"]