{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Kapaciteti ftohës","Kapaciteti total","","Nom.","kW","12.10","19.00","22.00"]
["Kapaciteti ngrohës","Kapaciteti total","","Nom.","kW","13.50","22.4","24.0"]
["Casing","Ngjyra","","","","Pa bojë","Pa bojë","Pa bojë"]
["","Material","","","","Çelik i galvanizuar","Pllakë çeliku e galvanizuar","Pllakë çeliku e galvanizuar"]
["Dimensionet","Njësia","","Lartësia","mm","300","470","470"]
["","","","Gjerësia","mm","1,400","1,490","1,490"]
["","","","Thellësia","mm","700","1,100","1,100"]
["Pesha","Njësia","","","kg","45","104","115"]
["Boshllëku i kërkuar i tavanit >","mm","","","","350"]
["Fan","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50","56"]
["","","","I ulët","m³/min","28.0","36.0","43.0"]
["","","Ngrohje","I lartë","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50.0","56.0"]
["","","","I ulët","m³/min","28.0","36.0","43.0"]
["","Presioni i jashtëm statik","","I lartë","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","66","69.0","71.0"]
["Niveli i presionit të zhurmës","Ftohje","","I lartë","dBA","40","43.0","44.0"]
["","","","Medium","dBA","","39.0","40.0"]
["","","","I ulët","dBA","33","36.0","37.0"]
["","Ngrohje","","I lartë","dBA","40","43.0","44.0"]
["","","","Mesatar","dBA","","39.0","40.0"]
["","","","I ulët","dBA","33","36.0","37.0"]
["Lidhjet e tubacioneve","Lëngu","","Diametri i jashtëm","mm","9.52","9.52","9.52"]
["","Gazi","","Diametri i jashtëm","mm","15.90","19.1","22.2"]
["","Kullimi","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Lartësia e kullimit","mm","","","","625"]
["Paneli i dekorimit","Model","","","","BYBS125DJW1"]
["","Ngjyra","","","","E bardhë (10Y9 / 0.5)"]
["","Dimensionet","","Lartësia","mm","55"]
["","","","Gjerësia","mm","1,500"]
["","","","Thellësia","mm","500"]
["","Pesha","","","kg","6.5"]
["Control systems","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Aksesore Standarde","Vida","","","","16","2","2"]
["","Rondele","","","","8","12","12"]
["","Fashetë","","","","1"]
["","Zorrë kullimi","","","","1"]
["","Masat e përgjithshme të sigurisë","","","","1","1","1"]
["","Manual instalimi dhe përdorimi","","","","1","1","1"]
["","Tel për furnizimin e përgjithshëm me energji","","","","2"]
["","Material izolues (zorrë shkarkimi)","","","","1"]
["","Material izolues","","","","2"]
["","Tub termoizolimi (lëng)","","","","1"]
["","Tub termoizolimi (gaz)","","","","1"]
["Power supply","Name","","","","","VE","VE"]
["","Faza","","","","1~","1~","1~"]
["","Frekuenca","","","Hz","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220"]
["Shënime","","","","","(1) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["Aksesore Standarde","Manual përdorimi","","","","","1","1"]
["","Manual instalimi","","","","","1","1"]
["","Tub për lidhjen e gazit","","","","","1","1"]
["","Material mbërthimi për tela","","","","","1","1"]
["","Rondelë me sustë","","","","","2","2"]
["","Vida+Rondela","","","","","45","45"]
["","Vidë me kokë hekzagon me rondelë","","","","","49","49"]
["","Vidë me kokë hekzagon","","","","","2","2"]
["","Rondelë e thjeshtë","","","","","8","8"]