{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-D3/D9V1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125D9V1B"]
["Kapaciteti ftohës","Nom.","","kW","12.5 (3)"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","9.52"]
["","Gazi","Dia. jasht.","mm","15.9"]
["","Kullimi","Diametri i jashtëm","mm","26"]
["Ftohja e hapësirës","SEER","","","3.50"]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","1,978"]
["","EER","","","3.16"]
["","COP","","","3.88"]
["","Direktiva e etiketimit të energjisë","Ftohje","","B"]
["","","Ngrohje","","A"]
["Kapaciteti ngrohës","Nom.","","kW","14.0 (4)"]
["Shënime","","","","(1) - Etiketa e energjisë: nga shkalla A (më efikasja) deri në G (më pak efikasja)"]
["","","","","(2) - Konsumi vjetor i energjisë: bazuar në përdorimin mesatar prej 500 orë pune në vit me ngarkesë të plotë (kushte nominale)."]
["","","","","(3) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 5m; diferenca e nivelit: 0m"]
["","","","","(4) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m; diferenca e nivelit: 0m"]
["","","","","(5) - Efikasiteti nominal: ftohje në ngarkesë nominale 35°/27°, ngrohje në ngarkesë nominale 7°/20°"]