{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RQ-BW1"]
[]
[]
[]
[]
["","","","","FHA71AVEB / RQ71B8W1B","FHA100AVEB / RQ100B8W1B","FHA125AVEB / RQ125B8W1B"]
["Kapaciteti ftohës","Nom.","","kW","7.10 (2)","9.80 (2)","12.2 (1)"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","9.52","9.52","9.52"]
["","Gas","Dia. jasht.","mm","15.9","15.9","15.9"]
["","Kullimi","Diametri i jashtëm","mm","26","26","26"]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","1,325","1,840","2,255"]
["","EER","","","2.68","2.66","2.71"]
["","COP","","","2.86","2.79","2.81"]
["","Direktiva e etiketimit të energjisë","Ftohje","","D","D","D"]
["","","Ngrohje","","D","E","D"]
["Kapaciteti ngrohës","Nom.","","kW","8.00 (3)","11.2 (3)","14.5 (3)"]
["Shënime","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m","(1) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7.5m (horizontalisht); diferenca e nivelit: 0m"]
["","","","","(2) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7.5m (horizontalisht); diferenca e nivelit: 0m","(2) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7.5m (horizontalisht); diferenca e nivelit: 0m","(2) - Ftohje: temp. e brendshme 27°CDB, 19°CWB; temp. e jashtme 35°CDB; gjatësia barazvlerëse e tubave: 7,5m; diferenca e nivelit: 0m"]
["","","","","(3) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(3) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m","(3) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 7,5m; diferenca e nivelit: 0m"]