{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Kapaciteti ftohës","Nom.","","kW","3.40"]
["Ftohja e hapësirës","SEER","","","6.24"]
["","Konsumi vjetor i energjisë","","kWh/a","191"]
["","Kapaciteti","Pdesign","kW","3.40"]
["","Kategoria e efikasitetit të energjisë","","","A++"]
["Ngrohja e hapësirës (klimë mesatare)","Kapaciteti","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Kategoria e efikasitetit të energjisë","","","A+"]
["","Konsumi vjetor i energjisë","","kWh/a","979"]
["Efikasiteti nominal","Konsumi vjetor i energjisë","","kWh","456"]
["","EER","","","3.73"]
["","COP","","","4.08"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","A"]
["Kapaciteti ngrohës","Nom.","","kW","4.00"]
["Shënime","","","","(1) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["","","","","(2) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","(3) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temp. e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","(4) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["Outdoor unit","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Kapaciteti ftohës","Nom.","","kW","","5.00","5.70"]
["Kapaciteti ngrohës","Nom.","","kW","","6.00","7.20"]
["Efikasiteti nominal","EER","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Konsumi vjetor i energjisë","","kWh","","780","867"]
["","Direktiva e etiketimit të energjisë","Ftohje","","","B","A"]
["","","Ngrohje","","","C","C"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","","A+","A+"]
["","Kapaciteti","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Konsumi vjetor i energjisë","","kWh/a","","295","328"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","","A","A"]
["","Kapaciteti","Pdesign","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","","3.85","4.08"]
["","Konsumi vjetor i energjisë","","kWh/a","","1578","1704"]