{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":12,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB"]
[]
[]
[]
[]
["","","","","","FHQ35CBVEB (Archived)","FHQ50CBVEB (Archived)","FHQ60CBVEB (Archived)","FHQ71CBVEB (Archived)","FHQ100CBVEB (Archived)","FHQ125CBVEB (Archived)","FHQ140CBVEB (Archived)"]
["Veshja e jashtme","Ngjyra","","","","E bardhë","E bardhë","E bardhë","E bardhë","E bardhë","E bardhë","E bardhë"]
["","Materiali","","","","Rezinë, fletë metalike","Rezinë, fletë metalike","Rezinë, fletë metalike","Rezinë, fletë metalike","Rezinë, fletë metalike","Rezinë, fletë metalike","Rezinë, fletë metalike"]
["Dimensionet","Njësia","","Lartësia","mm","235","235","235","235","235","235","235"]
["","","","Gjerësia","mm","960","960","1270","1270","1590","1590","1590"]
["","","","Thellësia","mm","690","690","690","690","690","690","690"]
["Pesha","Njësia","","","kg","24","25","31","32","38","38","38"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","14","15","19.5","20.5","28","31","34"]
["","","","Nom.","m³/min","11.5","12","15","17","24","27","29"]
["","","","I ulët","m³/min","10","10","11.5","14","20","23","24"]
["","","Ngrohje","I lartë","m³/min","14","15","19.5","20.5","28","31","34"]
["","","","Nom.","m³/min","11.5","12","15","17","24","27","29"]
["","","","I ulët","m³/min","10","10","11.5","14","20","23","24"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","53","54","54","55","60","62","64"]
["","Ngrohje","","","dBA","53","54","54","55","60","62","64"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","36","37","37","38","42","44","46"]
["","","","Nom.","dBA","34","35","35","36","38","41","42"]
["","","","I ulët","dBA","31","32","33","34","34","37","38"]
["","Ngrohje","","I lartë","dBA","36","37","37","38","42","44","46"]
["","","","Nom.","dBA","34","35","35","36","38","41","42"]
["","","","I ulët","dBA","31","32","33","34","34","37","38"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gazi","","Dia. jasht.","mm","9.5","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Kullimi","","","","VP20","VP20","VP20","VP20","VP20","VP20","VP20"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53"]
["","Telekomandë me tela","","","","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A","BRC1D52, BRC1E52A/B, BRC1E53A, BRC1E53B, BRC1E53C, BRC1E51A"]
["Furnizimi me energji","Faza","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50","50","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]