{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Niveli i presionit të zhurmës","Ngrohje","I lartë","dBA","46"]
["","","Funksionim pa zhurmë","dBA","30"]
["","","I ulët","dBA","33"]
["","Ftohje","Funksionim pa zhurmë","dBA","29"]
["","","I ulët","dBA","32"]
["","","I lartë","dBA","38"]
["","","Nom.","dBA","36"]
["","Ftohje","Nom.","dBA","35"]
["Aksesore Standarde","Manual instalimi","","","1"]
["","Manual përdorimi","","","1"]
["","Telekomandë me rreze infra të kuqe","","","1"]
["","Bateri AAA me qeliza të thata","","","2"]
["","Mbajtës telekomande","","","1"]
["","Pllakë montimi","","","1"]
["","Tub termoizolues (tubi i lëngut ftohës)","","","8"]
["","Filtër për pastrimin e ajrit","","","1"]
["","Filtër fotokatalitik për heqjen e erërave","","","1"]
["","Kapak anësor","","","2"]
["","Fashë lidhëse","","","4"]
["Sistemet e kontrollit","Infrared remote control","","","ARC433B67"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","6.35"]
["","Gazi","Dia. jasht.","mm","9.5"]
["","Kullimi","","","18"]
["Niveli i fuqisë së zhurmës","Ftohje","","dBA","53"]
["","Ngrohje","","dBA","59"]
["Dimensionet","Njësia","Gjerësia","mm","1,050"]
["","","Thellësia","mm","200"]
["","","Lartësia","mm","490"]
["Veshja e jashtme","Ngjyra","","","Bajame e bardhë"]
["Pesha","Njësia","","kg","16"]
["Power supply","Faza","","","1~"]
["","Frekuenca","","Hz","50"]
["","Emri","","","VM"]
["","Tensioni","","V","220-240"]
["Shënime","","","","(1) - 220V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240V"]
["","","","","(4) - Kur lidhet me njësinë e jashtme të sistemeve të shumëfishta, referohuni specifikimeve të njësisë së jashtme të shumëfishtë për t'u lidhur."]