{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-GV"]
[]
[]
[]
[]
["","","","","FTX50GV1B","FTX60GV1B","FTX71GV1B","FTX20GV1B (Archived)","FTX25GV1B (Archived)","FTX35GV1B (Archived)"]
["Niveli i presionit të zhurmës","Ngrohje","I lartë","dBA","42","44","46","39","40","41"]
["","","Funksionim pa zhurmë","dBA","30","32","34","25","25","26"]
["","","I ulët","dBA","33","35","37","28","28","29"]
["","Ftohje","Funksionim pa zhurmë","dBA","31","33","34","22","22","23"]
["","","I ulët","dBA","34","36","37","25","26","27"]
["","","I lartë","dBA","43","45","46","39","40","41"]
["","","Nom.","dBA","38","40","42","34","34","35"]
["","Ftohje","Nom.","dBA","39","41","42","33","33","34"]
["Aksesore Standarde","Filtër fotokatalitik me apatit titani për pastrimin e ajrit","","","2","2","2","2","2","2"]
["","Manual përdorimi","","","1","1","1","1","1","1"]
["","Manual instalimi","","","1","1","1","1","1","1"]
["","Telekomandë me valë","","","1","1","1","1","1","1"]
["","Bateri","","","2","2","2","2","2","2"]
["","Mbajtës telekomande","","","1","1","1","1","1","1"]
["","Pllakë montimi","","","1","1","1","1","1","1"]
["","Vida mbërthimi për njësinë e brendshme","","","2","2"]
["Control systems","Infrared remote control","","","ARC433B70","ARC433B70","ARC433B70"]
["Piping connections","Liquid","Dia. jasht.","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","Diametri i jashtëm","mm","12.7","12.7","15.9","9.52","9.52","9.52"]
["","Kullimi","","","18","18","18","18","18","18"]
["Fuqia në hyrje","Ftohje","Nom.","kW","0.034","0.040 (2), 0.040 (3), 0.040 (4)","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Ngrohje","Nom.","kW","0.036","0.045 (2), 0.045 (3), 0.045 (4)","0.060 (2), 0.060 (3), 0.06 (4)"]
["Niveli i fuqisë së zhurmës","Ftohje","","dBA","59","60","63","55","56","57"]
["","Ngrohje","","dBA","58","59","62","55","56","57"]
["Dimensionet","Njësia","Gjerësia","mm","1,050","1,050","1,050","770","770","770"]
["","","Thellësia","mm","238","238","238","198","198","198"]
["","","Lartësia","mm","290","290","290","283","283","283"]
["Veshja e jashtme","Colour","","","E bardhë","E bardhë","E bardhë","E bardhë","E bardhë","E bardhë"]
["Pesha","Njësia","","kg","12","12","12","7","7","7"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Frekuenca","","Hz","50","50","50","50","50","50"]
["","Name","","","V1","V1","V1","V1","V1","V1"]
["","Tensioni","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Shënime","","","","(1) - SL: Niveli pa zhurmë i ventiatorit të parametrave të niormës së qarkullimit të ajrit","(1) - SL: Niveli pa zhurmë i ventiatorit të parametrave të niormës së qarkullimit të ajrit","(1) - SL: Niveli pa zhurmë i ventiatorit të parametrave të niormës së qarkullimit të ajrit"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V"]
["Aksesore Standarde","Vida fiksuese për njësinë e brendshme (M4 x 12L)","","","","","2"]
["","Vidë mbërthimi për njësinë e brendshme","","","","","","2","2","2"]