{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BT / RXA-B9"]
[]
[]
[]
[]
["","","","","FTXA42B2V1BT / RXA42B5V1B9 (Archived)"]
["Njësia e jashtme","","","","RXA42B5V1B9"]
["Kapaciteti ftohës","Min.","","kW","1.70"]
["","Nom.","","kW","4.20"]
["","Maks.","","kW","5.00"]
["Kapaciteti ngrohës","Min.","","kW","1.70"]
["","Nom.","","kW","5.40"]
["","Maks.","","kW","6.00"]
["Efikasiteti nominal","EER","","","3.99"]
["","COP","","","4.12"]
["","Konsumi vjetor i energjisë","","kWh","526"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","A"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","A++"]
["","Kapaciteti","Pdesign","kW","4.20"]
["","SEER","","","7.50"]
["","Konsumi vjetor i energjisë","","kWh/a","196"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","A++"]
["","Kapaciteti","Pdesign","kW","3.80"]
["","SCOP/A","","","4.60"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","3.04"]
["","Konsumi vjetor i energjisë","","kWh/a","1156"]
["Gama e efikasitetit të energjisë","","","","A+++ ~ D"]