{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":93,"n_cols":10,"rows_kept":93,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CB"]
[]
[]
[]
[]
["","","","","","FTXA20C2V1BB","FTXA25C2V1BB","FTXA35C2V1BB","FTXA42C2V1BB","FTXA50C2V1BB"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.020"]
["","Ngrohje","","Nom.","kW","0.020"]
["Veshja e jashtme","Ngjyra","","","","E zezë"]
["Dimensionet","Njësia","","Lartësia","mm","295"]
["","","","Gjerësia","mm","798"]
["","","","Thellësia","mm","189"]
["Pesha","Njësia","","","kg","11.5"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","11.0"]
["","","","Mesatar","m³/min","8.2"]
["","","","I ulët","m³/min","6.1"]
["","","","Funksionim pa zhurmë","m³/min","4.6"]
["","","Ngrohje","I lartë","m³/min","10.9"]
["","","","Mesatar","m³/min","8.7"]
["","","","I ulët","m³/min","6.4"]
["","","","Funksionim pa zhurmë","m³/min","4.5"]
["Sound power level","Ftohje","","","dBA","57"]
["Niveli i presionit të zhurmës","Ftohje","","I lartë","dBA","39"]
["","","","Mesatar","dBA","32"]
["","","","I ulët","dBA","25"]
["","","","Funksionim pa zhurmë","dBA","19"]
["","Ngrohje","","I lartë","dBA","39"]
["","","","Mesatar","dBA","32"]
["","","","I ulët","dBA","25"]
["","","","Funksionim pa zhurmë","dBA","19"]
["Agjenti ftohës","GWP","","","","675.0"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35"]
["","Gazi","","Dia. jasht.","mm","9.50"]
["","Kullimi","","","","18"]
["Sisteme kontrolli","Infrared remote control","","","","ARC466A85"]
["","Wired remote control","","","","BRC073A1"]
["Aksesore Standarde","Manual instalimi","","","","1"]
["","Manual përdorimi","","","","1"]
["","Filtër ajri","","","","2"]
["","Telekomandë me rreze infra të kuqe","","","","1"]
["","Pllakë montimi telekomande","","","","1"]
["","Qese vidash","","","","1"]
["","Mbulesa e vidës","","","","2"]
["","Bateri AAA me qeliza të thata","","","","2"]
["","Masat e përgjithshme të sigurisë","","","","1"]
["Power supply","Emri","","","","V1"]
["","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","220-240"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","0.022","0.023","0.028","0.030"]
["","Ngrohje","","Nom.","kW","","0.02","0.22","0.036","0.039"]
["Veshja e jashtme","Ngjyra","","","","","E zezë","E zezë","E zezë","E zezë"]
["Dimensionet","Njësia","","Lartësia","mm","","295","295","295","295"]
["","","","Gjerësia","mm","","798","798","798","798"]
["","","","Thellësia","mm","","189","189","189","189"]
["Pesha","Njësia","","","kg","","11.5","11.5","11.5","11.5"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","","11.5","11.9","13.1","13.5"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","","8.6","8.6","9.8","10.4"]
["","","","I ulët","m³/min","","6.1","6.1","7.2","7.6"]
["","","","Funksionim pa zhurmë","m³/min","","4.6","4.6","4.6","5.2"]
["","","Ngrohje","I lartë","m³/min","","11.1","11.5","14.6","15.1"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","","9","9","10.5","11.1"]
["","","Ngrohje","I ulët","m³/min","","6.4","6.4","7.7","8.2"]
["","","","Funksionim pa zhurmë","m³/min","","4.5","4.5","5.2","5.7"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","57","60","60","60"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","40","41","45","46"]
["","","","Mesatar","dBA","","33","33","37","39"]
["","","","I ulët","dBA","","25","25","29","31"]
["","","","Funksionim pa zhurmë","dBA","","19","19","21","24"]
["","Ngrohje","","I lartë","dBA","","40","41","45","46"]
["","","","Mesatar","dBA","","33","33","37","42"]
["","","","I ulët","dBA","","25","25","29","33"]
["","","","Funksionim pa zhurmë","dBA","","19","19","21","24"]
["Agjenti ftohës","GWP","","","","","675","675","675","675.0"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","6.35","6.35","6.35","6.35"]
["","Gazi","","Dia. jasht.","mm","","9.5","9.5","9.5","12.70"]
["","Kullimi","","","","","18","18","18","18"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","","ARC466A85","ARC466A85","ARC466A85","ARC466A85"]
["","Telekomandë me tela","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Aksesore Standarde","Installation manual","","","","","1","1","1","1"]
["","Screw cover","","","","","2","2","2","2"]
["","AAA dry-cell batteries","","","","","2","2","2","2"]
["","General safety precautions","","","","","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1"]
["","Filtër ajri","","","","","2","2","2","2"]
["","Infrared remote control","","","","","1","1","1","1"]
["","Remote controller mounting plate","","","","","1","1","1","1"]
["","Screw bag","","","","","1","1","1","1"]
["Furnizimi me energji","Emri","","","","","V1","V1","V1","V1"]
["","Faza","","","","","1~","1~","1~","1~"]
["","Frekuenca","","","Hz","","50","50","50","50"]
["","Tensioni","","","V","","220-240","220-240","220-240","220-240"]
["Gama e efikasitetit të energjisë","","","","","","","A+++ ~ D"]