{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CW / RXA-A8"]
[]
[]
[]
[]
["","","","","FTXA20C2V1BW / RXA20A5V1B8","FTXA25C2V1BW / RXA25A5V1B8","FTXA35C2V1BW / RXA35A5V1B8"]
["Kapaciteti ftohës","Min.","","kW","","1.30","1.40"]
["","Nom.","","kW","","2.50","3.40"]
["","Maks.","","kW","","3.20","4.00"]
["Kapaciteti ngrohës","Min.","","kW","","1.30","1.40"]
["","Nom.","","kW","","2.80","4.00"]
["","Maks.","","kW","","4.70","5.20"]
["Efikasiteti nominal","Annual energy consumption","","kWh","","280","389"]
["","COP","","","","5.00","4.04"]
["","EER","","","","4.46","4.37"]
["","Direktiva e etiketimit të energjisë","Ftohje","","","A","A"]
["","","Ngrohje","","","A","A"]
["Shënime","","","","","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temperatura e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m.","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temperatura e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m.","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","","(3) - Shiko skicën e veçantë për diapazonin e funksionimit","(3) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["Kapaciteti ftohës","Min.","","kW","1.30"]
["","Nom.","","kW","2.00"]
["","Maks.","","kW","2.60"]
["Kapaciteti ngrohës","Min.","","kW","1.30"]
["","Nom.","","kW","2.50"]
["","Maks.","","kW","3.50"]
["Efikasiteti nominal","EER","","","4.70"]
["","COP","","","5.00"]
["","Konsumi vjetor i energjisë","","kWh","213"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","A"]
["Ftohja e hapësirës","Kategoria e efikasitetit të energjisë","","","A+++"]
["","Kapaciteti","Pdesign","kW","2.00"]
["","SEER","","","8.75"]
["","Konsumi vjetor i energjisë","","kWh/a","80"]
["Ngrohja e hapësirës (klimë mesatare)","Kategoria e efikasitetit të energjisë","","","A+++"]
["","Kapaciteti","Pdesign","kW","2.40"]
["","SCOP/A","","","5.15"]
["","Pdh Kapaciteti i ngrohjes në -10°","","kW","2.04"]
["","Konsumi vjetor i energjisë","","kWh/a","652"]