{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BS","FTXJ25MV1BS","FTXJ35MV1BS","FTXJ50MV1BS"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.023","0.023","0.033","0.033"]
["","Ngrohje","","Nom.","kW","0.031","0.033","0.042","0.043"]
["Veshja e jashtme","Ngjyra","","","","Argjend","Argjend","Argjend","Argjend"]
["Dimensionet","Njësia","","Lartësia","mm","303","303","303","303"]
["","","","Gjerësia","mm","998","998","998","998"]
["","","","Thellësia","mm","212","212","212","212"]
["Pesha","Njësia","","","kg","12","12","12","12"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","8.9","8.9","10.9","10.9"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","6.6","6.6","7.8","8.9"]
["","","","I ulët","m³/min","4.4","4.4","4.8","6.8"]
["","","","Funksionim pa zhurmë","m³/min","2.6","2.6","2.9","3.6"]
["","","Ngrohje","I lartë","m³/min","10.2","11.0","12.4","12.6"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","8.4","8.6","9.6","10.5"]
["","","Ngrohje","I ulët","m³/min","6.3","6.3","6.9","8.1"]
["","","","Funksionim pa zhurmë","m³/min","3.8","3.8","4.1","5.0"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","54","54","59","60"]
["","Ngrohje","","","dBA","56","56","59","60"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","38","38","45","46"]
["","","","Mesatar","dBA","32","32","34","40"]
["","","","I ulët","dBA","25","25","26","35"]
["","","","Funksionim pa zhurmë","dBA","19","19","20","25"]
["","Ngrohje","","I lartë","dBA","40","41","45","47"]
["","","","Mesatar","dBA","34","34","37","41"]
["","","","I ulët","dBA","28","28","29","35"]
["","","","Funksionim pa zhurmë","dBA","19","19","20","25"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35","6.35","6.35","6.35"]
["","Gazi","","Dia. jasht.","mm","9.50","9.50","9.50","12.70"]
["","Kullimi","","","","18","18","18","18"]
["Sistemet e kontrollit","Telekomandë me rreze infra të kuqe","","","","ARC466A9","ARC466A9","ARC466A9","ARC466A9"]
["Aksesore Standarde","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","Screw cover","","","","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Fixing screw for remote controller holder","","","","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2"]
["","Fixing screws for mounting plate","","","","5","5","5","5"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Furnizimi me energji","Emri","","","","V1","V1","V1","V1"]
["","Faza","","","","1~","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240","220-240"]
["Shënime","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]