{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / RXJ-N"]
[]
[]
[]
[]
["","","","","FTXJ50MV1BW / RXJ50N2V1B"]
["Kapaciteti ftohës","Min.","","kW","1.40"]
["","Maks.","","kW","5.50"]
["","Nom.","","kW","4.80"]
["Efikasiteti nominal","Annual energy consumption","","kWh","716"]
["","EER","","","3.35"]
["","COP","","","3.65"]
["","Direktiva e etiketimit të energjisë","Ftohje","","A"]
["","","Ngrohje","","A"]
["Kapaciteti ngrohës","Nom.","","kW","5.80"]
["","Min.","","kW","1.10"]
["","Maks.","","kW","7.00"]
["Shënime","","","","(1) - Kapacitetet nominale të ftohjes bazohen në: temperatura e brendshme: 27°CDB, 19°CWB, temp. e jashtme: 35°CDB, tubacioni i barasvlershëm i agjentit ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","(2) - Kapacitetet nominale të ngrohjes bazohen në: temperatura e brendshme: 20°CDB, temperatura e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m, diferenca e nivelit: 0m."]
["","","","","(3) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","(4) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]