{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Niveli i presionit të zhurmës","Ngrohje","","I lartë","dBA","45.0"]
["","","","Mesatar","dBA","31.0"]
["","","","Funksionim pa zhurmë","dBA","19.0"]
["","","","I ulët","dBA","22.0"]
["","Ftohje","","Medium","dBA","33.0"]
["","","","Funksionim pa zhurmë","dBA","21.0"]
["","","","I ulët","dBA","25.0"]
["","","","I lartë","dBA","45.0"]
["Aksesore Standarde","Manual instalimi","","","","1"]
["","Manual përdorimi","","","","1"]
["","Telekomandë me valë","","","","1"]
["","Bateri AAA me qeliza të thata","","","","2"]
["","Mbajtës telekomande","","","","1"]
["","Pllakë montimi","","","","1"]
["","Vida mbërthimi për njësinë e brendshme","","","","2"]
["","Filtri prej argjendi për grimcat","","","","1"]
["Control systems","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Lidhjet e tubacioneve","Lëngu","","Diametri i jashtëm","mm","6.35"]
["","Gazi","","Diametri i jashtëm","mm","9.50"]
["","Kullimi","","","","18"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.035"]
["","Ngrohje","","Nom.","kW","0.039"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","60.0"]
["","Ngrohje","","","dBA","61.0"]
["Dimensionet","Njësia","","Gjerësia","mm","778"]
["","","","Thellësia","mm","272"]
["","","","Lartësia","mm","295"]
["Casing","Ngjyra","","","","E bardhë"]
["Pesha","Njësia","","","kg","10.0"]
["Fan","Niveli i qarkullimit të ajrit","Ngrohje","I lartë","m³/min","12.5"]
["","","","I ulët","m³/min","4.9"]
["","","","Medium","m³/min","7.5"]
["","","","Funksionim pa zhurmë","m³/min","4.0"]
["","","Ftohje","I ulët","m³/min","5.3"]
["","","","Medium","m³/min","7.8"]
["","","","I lartë","m³/min","12.2"]
["","","","Funksionim pa zhurmë","m³/min","4.1"]
["Power supply","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Name","","","","V1"]
["","Voltage","","","V","220-240"]
["Shënime","","","","","(1) - Ftohje: temp. e brendshme 27°CDB, 19.0°CWB; temperatura e jashtme 35°CDB, 24°CWB; gjatësia barazvlerëse e tubave: 5m"]
["","","","","","(2) - Ngrohje: temp. e brendshme 20°CDB; temp. e jashtme 7°CDB, 6°CWB, gjatësia e tubave ftohës: 5m"]
["","","","","","(3) - Shiko skicat e veçantë për të dhënat e skicave elektrike"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","","0.053"]
["","Ngrohje","","Nom.","kW","","0.06"]
["Veshja e jashtme","Ngjyra","","","","","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","","299"]
["","","","Gjerësia","mm","","998"]
["","","","Thellësia","mm","","292"]
["Pesha","Njësia","","","kg","","14.5"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","","15.4"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","","9.5"]
["","","","I ulët","m³/min","","5.8"]
["","","","Funksionim pa zhurmë","m³/min","","4.6"]
["","","Ngrohje","I lartë","m³/min","","17.5"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","","10.5"]
["","","Ngrohje","I ulët","m³/min","","7.1"]
["","","","Funksionim pa zhurmë","m³/min","","5.9"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","","60"]
["","Ngrohje","","","dBA","","61"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","","46"]
["","","","Mesatar","dBA","","32"]
["","","","I ulët","dBA","","24"]
["","","","Funksionim pa zhurmë","dBA","","20"]
["","Ngrohje","","I lartë","dBA","","46"]
["","","","Mesatar","dBA","","31"]
["","","","I ulët","dBA","","22"]
["","","","Funksionim pa zhurmë","dBA","","19"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","","6.35"]
["","Gazi","","Dia. jasht.","mm","","9.5"]
["","Kullimi","","","","","18"]
["Control systems","Infrared remote control","","","","","ARC466A75"]
["Sistemet e kontrollit","Telekomandë me tela","","","","","BRC073A1"]
["Aksesore Standarde","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Furnizimi me energji","Emri","","","","","V1"]
["","Faza","","","","","1~"]
["","Frekuenca","","","Hz","","50"]
["","Tensioni","","","V","","220-240"]