{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-A"]
[]
[]
[]
[]
["","","","","","FVXTM30A3V1B"]
["Fuqia në hyrje","Ftohje","","Nom.","kW","0.02"]
["","Ngrohje","","Nom.","kW","0.03"]
["Veshja e jashtme","Ngjyra","","","","E bardhë"]
["Dimensionet","Njësia","","Lartësia","mm","600"]
["","","","Gjerësia","mm","750"]
["","","","Thellësia","mm","238"]
["Pesha","Njësia","","","kg","17"]
["Ventilatori","Niveli i qarkullimit të ajrit","Ftohje","I lartë","m³/min","9"]
["","Shkalla e qarkullimit të ajrit","Ftohje","Mesatar","m³/min","6.7"]
["","","","I ulët","m³/min","4.8"]
["","","","Funksionim pa zhurmë","m³/min","4"]
["","","Ngrohje","I lartë","m³/min","9.4"]
["","Shkalla e qarkullimit të ajrit","Ngrohje","Mesatar","m³/min","6.8"]
["","","Ngrohje","I ulët","m³/min","5.3"]
["","","","Funksionim pa zhurmë","m³/min","4"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","53"]
["","Ngrohje","","","dBA","53"]
["Niveli i presionit të zhurmës","Ftohje","","Niveli i presionit të zhurmës-=-Ftohje-=-I lartë-=-dBA","dBA","39"]
["","","","Mesatar","dBA","32"]
["","","","I ulët","dBA","25"]
["","","","Funksionim pa zhurmë","dBA","20"]
["","Ngrohje","","I lartë","dBA","39"]
["","","","Mesatar","dBA","32"]
["","","","I ulët","dBA","25"]
["","","","Funksionim pa zhurmë","dBA","19"]
["Agjenti ftohës","GWP","","","","675"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","6.35"]
["","Gazi","","Dia. jasht.","mm","9.5"]
["","Kullimi","","","","VP20 (I.D. 20/O.D. 26)"]
["Sistemet e kontrollit","Infrared remote control","","","","ARC466A66"]
["Sistemet e kontrollit","Telekomandë me tela","","","","BRC073A1"]
["Aksesore Standarde","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","2"]
["Furnizimi me energji","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","220-240"]