{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B"]
[]
[]
[]
[]
["","","","","","RXA42B2V1B","RXA50B2V1B","RXA50B5V1B"]
["Dimensionet","Njësia","","Lartësia","mm","734","734","734"]
["","","","Gjerësia","mm","870","870","954"]
["","","","Thellësia","mm","373","373","401"]
["Pesha","Njësia","","","kg","50","50","49"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Ngrohje","Ambienti","Min.","°CWB","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","48.0","48.0","48"]
["","Ngrohje","","Nom.","dBA","48.0","48.0","48"]
["Agjenti ftohës","Lloji","","","","R-32","R-32","R-32"]
["","Mbushja","","","kg","1.10","1.10","1.1"]
["","Mbushja","","","tCO2Eq","0.75","0.75","0.75"]
["","GWP","","","","675","675","675"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","30","30","30"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","20","20","20"]
["Aksesore Standarde","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Furnizimi me energji","Faza","","","","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240"]
["Kompresori","Lloji","","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Shënime","","","","","","","(1) - Shiko skicën e veçantë për diapazonin e funksionimit"]
["","","","","","","","(2) - Shiko skicën e veçantë për të dhënat e skicave elektrike"]
["","","","","","","","(3) - Përmban gaze të fluorinuara të efektit serrë"]