{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-N"]
[]
[]
[]
[]
["","","","","","RXJ50N2V1B"]
["Dimensionet","Njësia","","Lartësia","mm","734"]
["","","","Gjerësia","mm","870"]
["","","","Thellësia","mm","373"]
["Pesha","Njësia","","","kg","50"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-10"]
["","","","Maks.","°CDB","46"]
["","Ngrohje","Ambienti","Min.","°CWB","-15"]
["","","","Maks.","°CWB","18"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","48.0"]
["","Ngrohje","","Nom.","dBA","48.0"]
["Agjenti ftohës","Lloji","","","","R-32"]
["","Mbushja","","","kg","1.15"]
["","Mbushja","","","tCO2Eq","0.78"]
["","GWP","","","","675"]
["Lidhjet e tubacioneve","Gjatësia e tubacioneve","Maks.","OU - IU","m","30"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","0.02 (për gjatësinë e tubave që kalojnë 10m)"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","20"]
["Aksesore Standarde","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["Furnizimi me energji","Faza","","","","1~"]
["","Frekuenca","","","Hz","50"]
["","Tensioni","","","V","220-240"]