{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":13,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-NV1"]
[]
[]
[]
[]
["","","","","","RZAG71N7V1B","RZAG71N2V1B","RZAG100N7V1B","RZAG100N2V1B","RZAG125N7V1B","RZAG125N2V1B","RZAG140N7V1B","RZAG140N2V1B"]
["Dimensionet","Njësia","","Lartësia","mm","870","870","870","870","870","870","870","870"]
["","","","Gjerësia","mm","1100","1100","1100","1100","1100","1100","1100","1100"]
["","","","Thellësia","mm","460","460","460","460","460","460","460","460"]
["Pesha","Njësia","","","kg","81","81","85","85","95","95","95","95"]
["Kompresori","Type","","","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Diapazoni i funksionimit","Ftohje","Ambienti","Min.","°CDB","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Maks.","°CDB","52","52","52","52","52","52","52","52"]
["","Ngrohje","Ambienti","Min.","°CWB","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Maks.","°CWB","18","18","18","18","18","18","18","18"]
["Niveli i fuqisë së zhurmës","Ftohje","","","dBA","64","64","66","66","69","69","70","70"]
["","Ngrohje","","","dBA","","","","","68 (1)","68 (1)","71 (1)","71 (1)"]
["Niveli i presionit të zhurmës","Ftohje","","Nom.","dBA","46","46","47","47","49","49","50","50"]
["","Ngrohje","","Nom.","dBA","48","48","50","50","52","52","52","52"]
["Agjenti ftohës","Lloji","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Mbushja","","","kg","3.2","3.20","3.2","3.20","3.7","3.70","3.7","3.70"]
["","GWP","","","","675","675","675","675","675","675","675","675"]
["","Mbushja","","","tCO2Eq","2.16","2.16","2.16","2.16","2.5","2.50","2.5","2.50"]
["Lidhjet e tubacioneve","Lëngu","","Dia. jasht.","mm","10","10","10","10","10","10","10","10"]
["","Gazi","","Dia. jasht.","mm","15.9","15.9","15.9","15.9","15.9","15.9","15.9","15.9"]
["","Gjatësia e tubacioneve","Maks.","OU - IU","m","55","55","85","85","85","85","85","85"]
["","","Sistemi","Ekuivalent","m","75","75","100","100","100","100","100","100"]
["","","","Pa ngarkesë","m","40","40","40","40","40","40","40","40"]
["","Mbushje shtesë me agjent ftohës","","","kg/m","Shihni manualin e instalimit","Shihni manualin e instalimit","Shihni manualin e instalimit","Shihni manualin e instalimit","Shihni manualin e instalimit","Shihni manualin e instalimit","Shihni manualin e instalimit","Shihni manualin e instalimit"]
["","Ndryshimi i nivelit","IU - OU","Maks.","m","30","30","30","30","30","30","30","30"]
["","","IU - IU","Maks.","m","0.5","0.5","0.5","0.5","0.5","0.5","0.5","0.5"]
["Aksesore Standarde","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1","1"]
["","Peel off F-gas label","","","","1","1","1","1","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2","2","2","2","2"]
["Furnizimi me energji","Faza","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frekuenca","","","Hz","50","50","50","50","50","50","50","50"]
["","Tensioni","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Rryma - 50 Hz","Amperët maksimalë të siguresës (MFA)","","","A","20","20","32","32","32","32","32","32"]
["Kompresori","Lloji","","","","Kompresor rrotullues i mbyllur hermetikisht","Kompresor rrotullues i mbyllur hermetikisht"]
["Shënime","","","","","","","","","(1) - Sipas ENER Lot 21","(1) - Sipas ENER Lot 21","(1) - Sipas ENER Lot 21","(1) - Sipas ENER Lot 21"]