{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Niveli i presionit të zhurmës","Ngrohje","I lartë","dBA","38"]
["","","Mesatar","dBA","36"]
["","","I ulët","dBA","30"]
["","Ftohje","Mesatar","dBA","36"]
["","","I ulët","dBA","30"]
["","","I lartë","dBA","38"]
["Aksesore Standarde","Manual instalimi","","","1"]
["","Manual përdorimi","","","1"]
["","Izolues për rakorderi","","","1"]
["","Tampon izolues","","","1"]
["","Metal mbërthimi","","","1"]
["","Zorrë kullimi","","","1"]
["","Rondele për varëset","","","8"]
["","Material izolues","","","2"]
["","Mbërthyes","","","6"]
["","Pllakë fiksimi për rondelën","","","4"]
["","Vida për flanxhat e tubave","","","1"]
["","Filtër ajri","","","1"]
["Lidhjet e tubacioneve","Lëngu","Dia. jasht.","mm","6.35"]
["","Gas","Dia. jasht.","mm","12.7"]
["","Kullimi","","","VP20 (I.D. 20/O.D. 26)"]
["Fuqia në hyrje","Ftohje","Nom.","kW","0.060"]
["","Ngrohje","Nom.","kW","0.060"]
["Niveli i fuqisë së zhurmës","Ftohje","","dBA","55"]
["","Ngrohje","","dBA","55"]
["Dimensionet","Unit","Width","mm","1,150"]
["","","Thellësia","mm","620"]
["","","Height","mm","200"]
["Pesha","Njësia","","kg","30.0"]
["Ventilatori","Presioni i jashtëm statik","Nom.","Pa","40"]
["Power supply","Phase","","","1~"]
["","Frekuenca","","Hz","50/60"]
["","Emri","","","VE"]
["","Tensioni","","V","220-240"]
["Shënime","","","","(1) - Kur lidhet me njësinë e jashtme të sistemeve të shumëfishta, referohuni specifikimeve të njësisë së jashtme të shumëfishtë për t'u lidhur."]